Can_ErrorIrqCallback (uint8 u8Instance, Flexcan_Ip_EventType event, uint32 u32ErrStatus, const struct Flexcan_Ip_StateType * driverState)
{
  <bb 2> :
  if (event == 9)
    goto <bb 3>; [INV]
  else
    goto <bb 4>; [INV]

  <bb 3> :
<L0>:
  Can_ProcessBusOffInterrupt (u8Instance);
  goto <bb 5>; [INV]

  <bb 4> :
<L1>:

  <bb 5> :
  return;

}


Can_CommonIrqCallback (uint8 u8Instance, Flexcan_Ip_EventType event, uint32 u32buffIdx, const struct Flexcan_Ip_StateType * driverState)
{
  <bb 2> :
  if (event == 6)
    goto <bb 3>; [INV]
  else
    goto <bb 4>; [INV]

  <bb 3> :
  Can_ProcessPNInterrupt (u8Instance);

  <bb 4> :
  return;

}


