Trivially needed symbols: Uart_GetVersionInfo Uart_GetStatus Uart_AsyncSend Uart_AsyncReceive Uart_SyncReceive Uart_SyncSend Uart_SetBuffer Uart_Abort Uart_GetBaudrate Uart_SetBaudrate Uart_Deinit Uart_Init Uart_StartSetBuffer Uart_StartAsyncSend Uart_StartAsyncReceive Uart_StartSyncSend Uart_StartSyncReceive Uart_apConfig Uart_au32ClockFrequency Uart_au8DriverStatus


Initial Symbol table:

Uart_Ipw_AbortReceivingData/65 (Uart_Ipw_AbortReceivingData) @06e2f9a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_AbortSendingData/64 (Uart_Ipw_AbortSendingData) @06e2f8c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_GetBaudrate/63 (Uart_Ipw_GetBaudrate) @06e2f700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetBaudrate/40 
  Calls: 
Uart_Ipw_SetBaudrate/62 (Uart_Ipw_SetBaudrate) @06e2f540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_SetBaudrate/39 
  Calls: 
Uart_Ipw_Deinit/61 (Uart_Ipw_Deinit) @06e2f380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Deinit/38 
  Calls: 
Uart_Ipw_Init/60 (Uart_Ipw_Init) @06e2f1c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Init/37 
  Calls: 
Uart_pxPBcfgVariantPredefined/59 (Uart_pxPBcfgVariantPredefined) @06e32000
  Type: variable
  Visibility: external public
  References: 
  Referring: Uart_Init/37 (read)
  Availability: not-ready
  Varpool flags: read-only
Uart_Ipw_SetRxBuffer/58 (Uart_Ipw_SetRxBuffer) @06da1ee0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_SetTxBuffer/57 (Uart_Ipw_SetTxBuffer) @06da1e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_AsyncSend/56 (Uart_Ipw_AsyncSend) @06da1c40
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartAsyncSend/35 
  Calls: 
Uart_Ipw_AsyncReceive/55 (Uart_Ipw_AsyncReceive) @06da1a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartAsyncReceive/34 
  Calls: 
Uart_Ipw_SyncSend/54 (Uart_Ipw_SyncSend) @06da18c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncSend/33 
  Calls: 
Uart_Ipw_GetTransmitStatus/53 (Uart_Ipw_GetTransmitStatus) @06da17e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncSend/35 Uart_StartSyncSend/33 
  Calls: 
Det_ReportRuntimeError/52 (Det_ReportRuntimeError) @06da1620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_SyncReceive/51 (Uart_Ipw_SyncReceive) @06da1540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncReceive/32 
  Calls: 
Det_ReportError/50 (Det_ReportError) @06da1460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetVersionInfo/48 Uart_GetStatus/47 Uart_GetStatus/47 Uart_GetStatus/47 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_Abort/41 Uart_Abort/41 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_Deinit/38 Uart_Init/37 Uart_Init/37 Uart_StartAsyncSend/35 Uart_StartAsyncReceive/34 Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_GetReceiveStatus/49 (Uart_Ipw_GetReceiveStatus) @06da1380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncReceive/34 Uart_StartSyncReceive/32 
  Calls: 
Uart_GetVersionInfo/48 (Uart_GetVersionInfo) @06d95d20
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @01733ea0
  References: 
  Referring: 
  Function flags: body
  Called by: 
  Calls: Det_ReportError/50 
Uart_GetStatus/47 (Uart_GetStatus) @06d957e0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d95d20
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetReceiveStatus/49 Uart_Ipw_GetTransmitStatus/53 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncSend/46 (Uart_AsyncSend) @06d952a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d957e0
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncSend/35 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncReceive/45 (Uart_AsyncReceive) @06d95ee0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d952a0
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncReceive/34 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncReceive/44 (Uart_SyncReceive) @06d95c40
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d95ee0
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncReceive/32 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncSend/43 (Uart_SyncSend) @06d959a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d95c40
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncSend/33 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBuffer/42 (Uart_SetBuffer) @06d95700
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d959a0
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSetBuffer/36 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_Abort/41 (Uart_Abort) @06d95460
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d95700
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_AbortReceivingData/65 Uart_Ipw_AbortSendingData/64 Det_ReportError/50 Det_ReportError/50 
Uart_GetBaudrate/40 (Uart_GetBaudrate) @06d951c0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d95460
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetBaudrate/63 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBaudrate/39 (Uart_SetBaudrate) @06d8dee0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d951c0
  References: Uart_au8DriverStatus/29 (read)Uart_au32ClockFrequency/30 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_SetBaudrate/62 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 Uart_Ipw_GetReceiveStatus/49 Det_ReportError/50 Det_ReportError/50 
Uart_Deinit/38 (Uart_Deinit) @06d8d9a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d8dee0
  References: Uart_au8DriverStatus/29 (read)Uart_apConfig/31 (read)Uart_au8DriverStatus/29 (write)Uart_apConfig/31 (write)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Deinit/61 Det_ReportError/50 
Uart_Init/37 (Uart_Init) @06d8d460
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  Aux: @06d8d9a0
  References: Uart_au8DriverStatus/29 (read)Uart_pxPBcfgVariantPredefined/59 (read)Uart_apConfig/31 (write)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_au32ClockFrequency/30 (write)Uart_au8DriverStatus/29 (write)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Init/60 Det_ReportError/50 Det_ReportError/50 
Uart_StartSetBuffer/36 (Uart_StartSetBuffer) @06d8de00
  Type: function definition analyzed
  Visibility: force_output no_reorder
  Aux: @06d8d460
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SetBuffer/42 
  Calls: Uart_Ipw_SetRxBuffer/58 Uart_Ipw_SetTxBuffer/57 
Uart_StartAsyncSend/35 (Uart_StartAsyncSend) @06d8db60
  Type: function definition analyzed
  Visibility: force_output no_reorder
  Aux: @06d8de00
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_AsyncSend/46 
  Calls: Uart_Ipw_AsyncSend/56 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartAsyncReceive/34 (Uart_StartAsyncReceive) @06d8d8c0
  Type: function definition analyzed
  Visibility: force_output no_reorder
  Aux: @06d8db60
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_AsyncReceive/45 
  Calls: Uart_Ipw_AsyncReceive/55 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_StartSyncSend/33 (Uart_StartSyncSend) @06d8d620
  Type: function definition analyzed
  Visibility: force_output no_reorder
  Aux: @06d8d8c0
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SyncSend/43 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncSend/54 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartSyncReceive/32 (Uart_StartSyncReceive) @06d8d380
  Type: function definition analyzed
  Visibility: force_output no_reorder
  Aux: @06d8d620
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SyncReceive/44 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncReceive/51 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_apConfig/31 (Uart_apConfig) @06cb8318
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  Aux: @06d8d380
  References: 
  Referring: Uart_Init/37 (write)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Deinit/38 (read)Uart_Deinit/38 (write)
  Availability: not-ready
  Varpool flags:
Uart_au32ClockFrequency/30 (Uart_au32ClockFrequency) @06cb8240
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  Aux: @06cb8318
  References: 
  Referring: Uart_Init/37 (write)Uart_SetBaudrate/39 (read)
  Availability: not-ready
  Varpool flags:
Uart_au8DriverStatus/29 (Uart_au8DriverStatus) @06cb81b0
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  Aux: @06cb8240
  References: 
  Referring: Uart_Init/37 (read)Uart_Init/37 (write)Uart_Deinit/38 (read)Uart_Deinit/38 (write)Uart_SetBaudrate/39 (read)Uart_GetBaudrate/40 (read)Uart_Abort/41 (read)Uart_SetBuffer/42 (read)Uart_SyncSend/43 (read)Uart_SyncReceive/44 (read)Uart_AsyncReceive/45 (read)Uart_AsyncSend/46 (read)Uart_GetStatus/47 (read)
  Availability: not-ready
  Varpool flags:
Lpuart_Uart_Ip_FlushRxBuffer/28 (Lpuart_Uart_Ip_FlushRxBuffer) @06ca42a0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_FlushTxBuffer/27 (Lpuart_Uart_Ip_FlushTxBuffer) @06ca4000
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_CheckTimeout/26 (Lpuart_Uart_Ip_CheckTimeout) @06c9fd20
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_StartTimeout/25 (Lpuart_Uart_Ip_StartTimeout) @06c9fa80
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_ClearErrorFlags/24 (Lpuart_Uart_Ip_ClearErrorFlags) @06c9f7e0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_ClearStatusFlagWithMask/23 (Lpuart_Uart_Ip_ClearStatusFlagWithMask) @06c9f540
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_ClearStatusFlag/22 (Lpuart_Uart_Ip_ClearStatusFlag) @06c9f2a0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_GetStatusFlag/21 (Lpuart_Uart_Ip_GetStatusFlag) @06c9f000
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_Getchar10/20 (Lpuart_Uart_Ip_Getchar10) @06c96d20
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_Getchar9/19 (Lpuart_Uart_Ip_Getchar9) @06c96a80
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_Getchar/18 (Lpuart_Uart_Ip_Getchar) @06c967e0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_Putchar10/17 (Lpuart_Uart_Ip_Putchar10) @06c96540
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_Putchar9/16 (Lpuart_Uart_Ip_Putchar9) @06c962a0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_Putchar/15 (Lpuart_Uart_Ip_Putchar) @06c96000
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetRxDmaCmd/14 (Lpuart_Uart_Ip_SetRxDmaCmd) @06c92d20
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetTxDmaCmd/13 (Lpuart_Uart_Ip_SetTxDmaCmd) @06c92a80
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_GetIntMode/12 (Lpuart_Uart_Ip_GetIntMode) @06c927e0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetIntMode/11 (Lpuart_Uart_Ip_SetIntMode) @06c92540
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetStopBitCount/10 (Lpuart_Uart_Ip_SetStopBitCount) @06c922a0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetParityMode/9 (Lpuart_Uart_Ip_SetParityMode) @06c92000
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetBitCountPerChar/8 (Lpuart_Uart_Ip_SetBitCountPerChar) @06c8dd20
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_EnableBothEdgeSamplingCmd/7 (Lpuart_Uart_Ip_EnableBothEdgeSamplingCmd) @06c8da80
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_GetOversamplingRatio/6 (Lpuart_Uart_Ip_GetOversamplingRatio) @06c8d7e0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetOversamplingRatio/5 (Lpuart_Uart_Ip_SetOversamplingRatio) @06c8d540
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_GetBaudRateDivisor/4 (Lpuart_Uart_Ip_GetBaudRateDivisor) @06c8d1c0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetBaudRateDivisor/3 (Lpuart_Uart_Ip_SetBaudRateDivisor) @06beeee0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetReceiverCmd/2 (Lpuart_Uart_Ip_SetReceiverCmd) @06beec40
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_SetTransmitterCmd/1 (Lpuart_Uart_Ip_SetTransmitterCmd) @06bee9a0
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 
Lpuart_Uart_Ip_Hw_Init/0 (Lpuart_Uart_Ip_Hw_Init) @06bee700
  Type: function definition
  Visibility: no_reorder
  References: 
  Referring: 
  Function flags:
  Called by: 
  Calls: 

Removing unused symbols: Lpuart_Uart_Ip_FlushRxBuffer Lpuart_Uart_Ip_FlushTxBuffer Lpuart_Uart_Ip_CheckTimeout Lpuart_Uart_Ip_StartTimeout Lpuart_Uart_Ip_ClearErrorFlags Lpuart_Uart_Ip_ClearStatusFlagWithMask Lpuart_Uart_Ip_ClearStatusFlag Lpuart_Uart_Ip_GetStatusFlag Lpuart_Uart_Ip_Getchar10 Lpuart_Uart_Ip_Getchar9 Lpuart_Uart_Ip_Getchar Lpuart_Uart_Ip_Putchar10 Lpuart_Uart_Ip_Putchar9 Lpuart_Uart_Ip_Putchar Lpuart_Uart_Ip_SetRxDmaCmd Lpuart_Uart_Ip_SetTxDmaCmd Lpuart_Uart_Ip_GetIntMode Lpuart_Uart_Ip_SetIntMode Lpuart_Uart_Ip_SetStopBitCount Lpuart_Uart_Ip_SetParityMode Lpuart_Uart_Ip_SetBitCountPerChar Lpuart_Uart_Ip_EnableBothEdgeSamplingCmd Lpuart_Uart_Ip_GetOversamplingRatio Lpuart_Uart_Ip_SetOversamplingRatio Lpuart_Uart_Ip_GetBaudRateDivisor Lpuart_Uart_Ip_SetBaudRateDivisor Lpuart_Uart_Ip_SetReceiverCmd Lpuart_Uart_Ip_SetTransmitterCmd Lpuart_Uart_Ip_Hw_Init

Reclaimed Symbol table:

Uart_Ipw_AbortReceivingData/65 (Uart_Ipw_AbortReceivingData) @06e2f9a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_AbortSendingData/64 (Uart_Ipw_AbortSendingData) @06e2f8c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_GetBaudrate/63 (Uart_Ipw_GetBaudrate) @06e2f700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetBaudrate/40 
  Calls: 
Uart_Ipw_SetBaudrate/62 (Uart_Ipw_SetBaudrate) @06e2f540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_SetBaudrate/39 
  Calls: 
Uart_Ipw_Deinit/61 (Uart_Ipw_Deinit) @06e2f380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Deinit/38 
  Calls: 
Uart_Ipw_Init/60 (Uart_Ipw_Init) @06e2f1c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Init/37 
  Calls: 
Uart_pxPBcfgVariantPredefined/59 (Uart_pxPBcfgVariantPredefined) @06e32000
  Type: variable
  Visibility: external public
  References: 
  Referring: Uart_Init/37 (read)
  Availability: not-ready
  Varpool flags: read-only
Uart_Ipw_SetRxBuffer/58 (Uart_Ipw_SetRxBuffer) @06da1ee0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_SetTxBuffer/57 (Uart_Ipw_SetTxBuffer) @06da1e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_AsyncSend/56 (Uart_Ipw_AsyncSend) @06da1c40
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartAsyncSend/35 
  Calls: 
Uart_Ipw_AsyncReceive/55 (Uart_Ipw_AsyncReceive) @06da1a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartAsyncReceive/34 
  Calls: 
Uart_Ipw_SyncSend/54 (Uart_Ipw_SyncSend) @06da18c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncSend/33 
  Calls: 
Uart_Ipw_GetTransmitStatus/53 (Uart_Ipw_GetTransmitStatus) @06da17e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncSend/35 Uart_StartSyncSend/33 
  Calls: 
Det_ReportRuntimeError/52 (Det_ReportRuntimeError) @06da1620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_SyncReceive/51 (Uart_Ipw_SyncReceive) @06da1540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncReceive/32 
  Calls: 
Det_ReportError/50 (Det_ReportError) @06da1460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetVersionInfo/48 Uart_GetStatus/47 Uart_GetStatus/47 Uart_GetStatus/47 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_Abort/41 Uart_Abort/41 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_Deinit/38 Uart_Init/37 Uart_Init/37 Uart_StartAsyncSend/35 Uart_StartAsyncReceive/34 Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_GetReceiveStatus/49 (Uart_Ipw_GetReceiveStatus) @06da1380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncReceive/34 Uart_StartSyncReceive/32 
  Calls: 
Uart_GetVersionInfo/48 (Uart_GetVersionInfo) @06d95d20
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: 
  Referring: 
  Function flags: body
  Called by: 
  Calls: Det_ReportError/50 
Uart_GetStatus/47 (Uart_GetStatus) @06d957e0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetReceiveStatus/49 Uart_Ipw_GetTransmitStatus/53 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncSend/46 (Uart_AsyncSend) @06d952a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncSend/35 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncReceive/45 (Uart_AsyncReceive) @06d95ee0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncReceive/34 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncReceive/44 (Uart_SyncReceive) @06d95c40
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncReceive/32 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncSend/43 (Uart_SyncSend) @06d959a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncSend/33 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBuffer/42 (Uart_SetBuffer) @06d95700
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSetBuffer/36 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_Abort/41 (Uart_Abort) @06d95460
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_AbortReceivingData/65 Uart_Ipw_AbortSendingData/64 Det_ReportError/50 Det_ReportError/50 
Uart_GetBaudrate/40 (Uart_GetBaudrate) @06d951c0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetBaudrate/63 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBaudrate/39 (Uart_SetBaudrate) @06d8dee0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_au32ClockFrequency/30 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_SetBaudrate/62 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 Uart_Ipw_GetReceiveStatus/49 Det_ReportError/50 Det_ReportError/50 
Uart_Deinit/38 (Uart_Deinit) @06d8d9a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_apConfig/31 (read)Uart_au8DriverStatus/29 (write)Uart_apConfig/31 (write)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Deinit/61 Det_ReportError/50 
Uart_Init/37 (Uart_Init) @06d8d460
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_pxPBcfgVariantPredefined/59 (read)Uart_apConfig/31 (write)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_au32ClockFrequency/30 (write)Uart_au8DriverStatus/29 (write)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Init/60 Det_ReportError/50 Det_ReportError/50 
Uart_StartSetBuffer/36 (Uart_StartSetBuffer) @06d8de00
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SetBuffer/42 
  Calls: Uart_Ipw_SetRxBuffer/58 Uart_Ipw_SetTxBuffer/57 
Uart_StartAsyncSend/35 (Uart_StartAsyncSend) @06d8db60
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_AsyncSend/46 
  Calls: Uart_Ipw_AsyncSend/56 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartAsyncReceive/34 (Uart_StartAsyncReceive) @06d8d8c0
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_AsyncReceive/45 
  Calls: Uart_Ipw_AsyncReceive/55 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_StartSyncSend/33 (Uart_StartSyncSend) @06d8d620
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SyncSend/43 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncSend/54 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartSyncReceive/32 (Uart_StartSyncReceive) @06d8d380
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SyncReceive/44 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncReceive/51 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_apConfig/31 (Uart_apConfig) @06cb8318
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (write)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Deinit/38 (read)Uart_Deinit/38 (write)
  Availability: not-ready
  Varpool flags:
Uart_au32ClockFrequency/30 (Uart_au32ClockFrequency) @06cb8240
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (write)Uart_SetBaudrate/39 (read)
  Availability: not-ready
  Varpool flags:
Uart_au8DriverStatus/29 (Uart_au8DriverStatus) @06cb81b0
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (read)Uart_Init/37 (write)Uart_Deinit/38 (read)Uart_Deinit/38 (write)Uart_SetBaudrate/39 (read)Uart_GetBaudrate/40 (read)Uart_Abort/41 (read)Uart_SetBuffer/42 (read)Uart_SyncSend/43 (read)Uart_SyncReceive/44 (read)Uart_AsyncReceive/45 (read)Uart_AsyncSend/46 (read)Uart_GetStatus/47 (read)
  Availability: not-ready
  Varpool flags:


Initial Symbol table:

Uart_Ipw_AbortReceivingData/65 (Uart_Ipw_AbortReceivingData) @06e2f9a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_AbortSendingData/64 (Uart_Ipw_AbortSendingData) @06e2f8c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_GetBaudrate/63 (Uart_Ipw_GetBaudrate) @06e2f700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetBaudrate/40 
  Calls: 
Uart_Ipw_SetBaudrate/62 (Uart_Ipw_SetBaudrate) @06e2f540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_SetBaudrate/39 
  Calls: 
Uart_Ipw_Deinit/61 (Uart_Ipw_Deinit) @06e2f380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Deinit/38 
  Calls: 
Uart_Ipw_Init/60 (Uart_Ipw_Init) @06e2f1c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Init/37 
  Calls: 
Uart_pxPBcfgVariantPredefined/59 (Uart_pxPBcfgVariantPredefined) @06e32000
  Type: variable
  Visibility: external public
  References: 
  Referring: Uart_Init/37 (read)
  Availability: not-ready
  Varpool flags: read-only
Uart_Ipw_SetRxBuffer/58 (Uart_Ipw_SetRxBuffer) @06da1ee0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_SetTxBuffer/57 (Uart_Ipw_SetTxBuffer) @06da1e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_AsyncSend/56 (Uart_Ipw_AsyncSend) @06da1c40
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartAsyncSend/35 
  Calls: 
Uart_Ipw_AsyncReceive/55 (Uart_Ipw_AsyncReceive) @06da1a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartAsyncReceive/34 
  Calls: 
Uart_Ipw_SyncSend/54 (Uart_Ipw_SyncSend) @06da18c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncSend/33 
  Calls: 
Uart_Ipw_GetTransmitStatus/53 (Uart_Ipw_GetTransmitStatus) @06da17e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncSend/35 Uart_StartSyncSend/33 
  Calls: 
Det_ReportRuntimeError/52 (Det_ReportRuntimeError) @06da1620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_SyncReceive/51 (Uart_Ipw_SyncReceive) @06da1540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncReceive/32 
  Calls: 
Det_ReportError/50 (Det_ReportError) @06da1460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetVersionInfo/48 Uart_GetStatus/47 Uart_GetStatus/47 Uart_GetStatus/47 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_Abort/41 Uart_Abort/41 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_Deinit/38 Uart_Init/37 Uart_Init/37 Uart_StartAsyncSend/35 Uart_StartAsyncReceive/34 Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_GetReceiveStatus/49 (Uart_Ipw_GetReceiveStatus) @06da1380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncReceive/34 Uart_StartSyncReceive/32 
  Calls: 
Uart_GetVersionInfo/48 (Uart_GetVersionInfo) @06d95d20
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: 
  Referring: 
  Function flags: body
  Called by: 
  Calls: Det_ReportError/50 
Uart_GetStatus/47 (Uart_GetStatus) @06d957e0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetReceiveStatus/49 Uart_Ipw_GetTransmitStatus/53 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncSend/46 (Uart_AsyncSend) @06d952a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncSend/35 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncReceive/45 (Uart_AsyncReceive) @06d95ee0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncReceive/34 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncReceive/44 (Uart_SyncReceive) @06d95c40
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncReceive/32 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncSend/43 (Uart_SyncSend) @06d959a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncSend/33 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBuffer/42 (Uart_SetBuffer) @06d95700
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSetBuffer/36 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_Abort/41 (Uart_Abort) @06d95460
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_AbortReceivingData/65 Uart_Ipw_AbortSendingData/64 Det_ReportError/50 Det_ReportError/50 
Uart_GetBaudrate/40 (Uart_GetBaudrate) @06d951c0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetBaudrate/63 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBaudrate/39 (Uart_SetBaudrate) @06d8dee0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_au32ClockFrequency/30 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_SetBaudrate/62 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 Uart_Ipw_GetReceiveStatus/49 Det_ReportError/50 Det_ReportError/50 
Uart_Deinit/38 (Uart_Deinit) @06d8d9a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_apConfig/31 (read)Uart_au8DriverStatus/29 (write)Uart_apConfig/31 (write)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Deinit/61 Det_ReportError/50 
Uart_Init/37 (Uart_Init) @06d8d460
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_pxPBcfgVariantPredefined/59 (read)Uart_apConfig/31 (write)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_au32ClockFrequency/30 (write)Uart_au8DriverStatus/29 (write)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Init/60 Det_ReportError/50 Det_ReportError/50 
Uart_StartSetBuffer/36 (Uart_StartSetBuffer) @06d8de00
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SetBuffer/42 
  Calls: Uart_Ipw_SetRxBuffer/58 Uart_Ipw_SetTxBuffer/57 
Uart_StartAsyncSend/35 (Uart_StartAsyncSend) @06d8db60
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_AsyncSend/46 
  Calls: Uart_Ipw_AsyncSend/56 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartAsyncReceive/34 (Uart_StartAsyncReceive) @06d8d8c0
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_AsyncReceive/45 
  Calls: Uart_Ipw_AsyncReceive/55 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_StartSyncSend/33 (Uart_StartSyncSend) @06d8d620
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SyncSend/43 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncSend/54 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartSyncReceive/32 (Uart_StartSyncReceive) @06d8d380
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SyncReceive/44 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncReceive/51 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_apConfig/31 (Uart_apConfig) @06cb8318
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (write)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Deinit/38 (read)Uart_Deinit/38 (write)
  Availability: not-ready
  Varpool flags:
Uart_au32ClockFrequency/30 (Uart_au32ClockFrequency) @06cb8240
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (write)Uart_SetBaudrate/39 (read)
  Availability: not-ready
  Varpool flags:
Uart_au8DriverStatus/29 (Uart_au8DriverStatus) @06cb81b0
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (read)Uart_Init/37 (write)Uart_Deinit/38 (read)Uart_Deinit/38 (write)Uart_SetBaudrate/39 (read)Uart_GetBaudrate/40 (read)Uart_Abort/41 (read)Uart_SetBuffer/42 (read)Uart_SyncSend/43 (read)Uart_SyncReceive/44 (read)Uart_AsyncReceive/45 (read)Uart_AsyncSend/46 (read)Uart_GetStatus/47 (read)
  Availability: not-ready
  Varpool flags:

Removing unused symbols:

Reclaimed Symbol table:

Uart_Ipw_AbortReceivingData/65 (Uart_Ipw_AbortReceivingData) @06e2f9a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_AbortSendingData/64 (Uart_Ipw_AbortSendingData) @06e2f8c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_GetBaudrate/63 (Uart_Ipw_GetBaudrate) @06e2f700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetBaudrate/40 
  Calls: 
Uart_Ipw_SetBaudrate/62 (Uart_Ipw_SetBaudrate) @06e2f540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_SetBaudrate/39 
  Calls: 
Uart_Ipw_Deinit/61 (Uart_Ipw_Deinit) @06e2f380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Deinit/38 
  Calls: 
Uart_Ipw_Init/60 (Uart_Ipw_Init) @06e2f1c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_Init/37 
  Calls: 
Uart_pxPBcfgVariantPredefined/59 (Uart_pxPBcfgVariantPredefined) @06e32000
  Type: variable
  Visibility: external public
  References: 
  Referring: Uart_Init/37 (read)
  Availability: not-ready
  Varpool flags: read-only
Uart_Ipw_SetRxBuffer/58 (Uart_Ipw_SetRxBuffer) @06da1ee0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_SetTxBuffer/57 (Uart_Ipw_SetTxBuffer) @06da1e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_AsyncSend/56 (Uart_Ipw_AsyncSend) @06da1c40
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartAsyncSend/35 
  Calls: 
Uart_Ipw_AsyncReceive/55 (Uart_Ipw_AsyncReceive) @06da1a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartAsyncReceive/34 
  Calls: 
Uart_Ipw_SyncSend/54 (Uart_Ipw_SyncSend) @06da18c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncSend/33 
  Calls: 
Uart_Ipw_GetTransmitStatus/53 (Uart_Ipw_GetTransmitStatus) @06da17e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncSend/35 Uart_StartSyncSend/33 
  Calls: 
Det_ReportRuntimeError/52 (Det_ReportRuntimeError) @06da1620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_SyncReceive/51 (Uart_Ipw_SyncReceive) @06da1540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_StartSyncReceive/32 
  Calls: 
Det_ReportError/50 (Det_ReportError) @06da1460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetVersionInfo/48 Uart_GetStatus/47 Uart_GetStatus/47 Uart_GetStatus/47 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_Abort/41 Uart_Abort/41 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_Deinit/38 Uart_Init/37 Uart_Init/37 Uart_StartAsyncSend/35 Uart_StartAsyncReceive/34 Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_GetReceiveStatus/49 (Uart_Ipw_GetReceiveStatus) @06da1380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncReceive/34 Uart_StartSyncReceive/32 
  Calls: 
Uart_GetVersionInfo/48 (Uart_GetVersionInfo) @06d95d20
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: 
  Referring: 
  Function flags: body
  Called by: 
  Calls: Det_ReportError/50 
Uart_GetStatus/47 (Uart_GetStatus) @06d957e0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetReceiveStatus/49 Uart_Ipw_GetTransmitStatus/53 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncSend/46 (Uart_AsyncSend) @06d952a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncSend/35 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncReceive/45 (Uart_AsyncReceive) @06d95ee0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncReceive/34 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncReceive/44 (Uart_SyncReceive) @06d95c40
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncReceive/32 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncSend/43 (Uart_SyncSend) @06d959a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncSend/33 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBuffer/42 (Uart_SetBuffer) @06d95700
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_StartSetBuffer/36 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_Abort/41 (Uart_Abort) @06d95460
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_AbortReceivingData/65 Uart_Ipw_AbortSendingData/64 Det_ReportError/50 Det_ReportError/50 
Uart_GetBaudrate/40 (Uart_GetBaudrate) @06d951c0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetBaudrate/63 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBaudrate/39 (Uart_SetBaudrate) @06d8dee0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_au32ClockFrequency/30 (read)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_SetBaudrate/62 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 Uart_Ipw_GetReceiveStatus/49 Det_ReportError/50 Det_ReportError/50 
Uart_Deinit/38 (Uart_Deinit) @06d8d9a0
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_apConfig/31 (read)Uart_au8DriverStatus/29 (write)Uart_apConfig/31 (write)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Deinit/61 Det_ReportError/50 
Uart_Init/37 (Uart_Init) @06d8d460
  Type: function definition analyzed
  Visibility: force_output no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_pxPBcfgVariantPredefined/59 (read)Uart_apConfig/31 (write)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_au32ClockFrequency/30 (write)Uart_au8DriverStatus/29 (write)
  Referring: 
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Init/60 Det_ReportError/50 Det_ReportError/50 
Uart_StartSetBuffer/36 (Uart_StartSetBuffer) @06d8de00
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SetBuffer/42 
  Calls: Uart_Ipw_SetRxBuffer/58 Uart_Ipw_SetTxBuffer/57 
Uart_StartAsyncSend/35 (Uart_StartAsyncSend) @06d8db60
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_AsyncSend/46 
  Calls: Uart_Ipw_AsyncSend/56 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartAsyncReceive/34 (Uart_StartAsyncReceive) @06d8d8c0
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_AsyncReceive/45 
  Calls: Uart_Ipw_AsyncReceive/55 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_StartSyncSend/33 (Uart_StartSyncSend) @06d8d620
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SyncSend/43 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncSend/54 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartSyncReceive/32 (Uart_StartSyncReceive) @06d8d380
  Type: function definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: 
  Function flags: body
  Called by: Uart_SyncReceive/44 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncReceive/51 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_apConfig/31 (Uart_apConfig) @06cb8318
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (write)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Deinit/38 (read)Uart_Deinit/38 (write)
  Availability: not-ready
  Varpool flags:
Uart_au32ClockFrequency/30 (Uart_au32ClockFrequency) @06cb8240
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (write)Uart_SetBaudrate/39 (read)
  Availability: not-ready
  Varpool flags:
Uart_au8DriverStatus/29 (Uart_au8DriverStatus) @06cb81b0
  Type: variable definition analyzed
  Visibility: force_output no_reorder
  References: 
  Referring: Uart_Init/37 (read)Uart_Init/37 (write)Uart_Deinit/38 (read)Uart_Deinit/38 (write)Uart_SetBaudrate/39 (read)Uart_GetBaudrate/40 (read)Uart_Abort/41 (read)Uart_SetBuffer/42 (read)Uart_SyncSend/43 (read)Uart_SyncReceive/44 (read)Uart_AsyncReceive/45 (read)Uart_AsyncSend/46 (read)Uart_GetStatus/47 (read)
  Availability: not-ready
  Varpool flags:

Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Optimized Symbol table:

Uart_Ipw_AbortReceivingData/65 (Uart_Ipw_AbortReceivingData) @06e2f9a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_AbortSendingData/64 (Uart_Ipw_AbortSendingData) @06e2f8c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_Abort/41 
  Calls: 
Uart_Ipw_GetBaudrate/63 (Uart_Ipw_GetBaudrate) @06e2f700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_GetBaudrate/40 
  Calls: 
Uart_Ipw_SetBaudrate/62 (Uart_Ipw_SetBaudrate) @06e2f540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_SetBaudrate/39 
  Calls: 
Uart_Ipw_Deinit/61 (Uart_Ipw_Deinit) @06e2f380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_Deinit/38 
  Calls: 
Uart_Ipw_Init/60 (Uart_Ipw_Init) @06e2f1c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_Init/37 
  Calls: 
Uart_pxPBcfgVariantPredefined/59 (Uart_pxPBcfgVariantPredefined) @06e32000
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: Uart_Init/37 (read)
  Availability: not_available
  Varpool flags: read-only
Uart_Ipw_SetRxBuffer/58 (Uart_Ipw_SetRxBuffer) @06da1ee0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_SetTxBuffer/57 (Uart_Ipw_SetTxBuffer) @06da1e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_StartSetBuffer/36 
  Calls: 
Uart_Ipw_AsyncSend/56 (Uart_Ipw_AsyncSend) @06da1c40
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_StartAsyncSend/35 
  Calls: 
Uart_Ipw_AsyncReceive/55 (Uart_Ipw_AsyncReceive) @06da1a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_StartAsyncReceive/34 
  Calls: 
Uart_Ipw_SyncSend/54 (Uart_Ipw_SyncSend) @06da18c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_StartSyncSend/33 
  Calls: 
Uart_Ipw_GetTransmitStatus/53 (Uart_Ipw_GetTransmitStatus) @06da17e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncSend/35 Uart_StartSyncSend/33 
  Calls: 
Det_ReportRuntimeError/52 (Det_ReportRuntimeError) @06da1620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_SyncReceive/51 (Uart_Ipw_SyncReceive) @06da1540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_StartSyncReceive/32 
  Calls: 
Det_ReportError/50 (Det_ReportError) @06da1460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_GetVersionInfo/48 Uart_GetStatus/47 Uart_GetStatus/47 Uart_GetStatus/47 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncSend/46 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_AsyncReceive/45 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncReceive/44 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SyncSend/43 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_SetBuffer/42 Uart_Abort/41 Uart_Abort/41 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_GetBaudrate/40 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_SetBaudrate/39 Uart_Deinit/38 Uart_Init/37 Uart_Init/37 Uart_StartAsyncSend/35 Uart_StartAsyncReceive/34 Uart_StartSyncSend/33 Uart_StartSyncReceive/32 
  Calls: 
Uart_Ipw_GetReceiveStatus/49 (Uart_Ipw_GetReceiveStatus) @06da1380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Uart_GetStatus/47 Uart_SetBaudrate/39 Uart_StartAsyncReceive/34 Uart_StartSyncReceive/32 
  Calls: 
Uart_GetVersionInfo/48 (Uart_GetVersionInfo) @06d95d20
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Det_ReportError/50 
Uart_GetStatus/47 (Uart_GetStatus) @06d957e0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetReceiveStatus/49 Uart_Ipw_GetTransmitStatus/53 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncSend/46 (Uart_AsyncSend) @06d952a0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncSend/35 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_AsyncReceive/45 (Uart_AsyncReceive) @06d95ee0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_StartAsyncReceive/34 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncReceive/44 (Uart_SyncReceive) @06d95c40
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncReceive/32 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SyncSend/43 (Uart_SyncSend) @06d959a0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_StartSyncSend/33 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBuffer/42 (Uart_SetBuffer) @06d95700
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_StartSetBuffer/36 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_Abort/41 (Uart_Abort) @06d95460
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_AbortReceivingData/65 Uart_Ipw_AbortSendingData/64 Det_ReportError/50 Det_ReportError/50 
Uart_GetBaudrate/40 (Uart_GetBaudrate) @06d951c0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_GetBaudrate/63 Det_ReportError/50 Det_ReportError/50 Det_ReportError/50 
Uart_SetBaudrate/39 (Uart_SetBaudrate) @06d8dee0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_au32ClockFrequency/30 (read)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_SetBaudrate/62 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 Uart_Ipw_GetReceiveStatus/49 Det_ReportError/50 Det_ReportError/50 
Uart_Deinit/38 (Uart_Deinit) @06d8d9a0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_apConfig/31 (read)Uart_au8DriverStatus/29 (write)Uart_apConfig/31 (write)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Deinit/61 Det_ReportError/50 
Uart_Init/37 (Uart_Init) @06d8d460
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: Uart_au8DriverStatus/29 (read)Uart_pxPBcfgVariantPredefined/59 (read)Uart_apConfig/31 (write)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_apConfig/31 (read)Uart_au32ClockFrequency/30 (write)Uart_au8DriverStatus/29 (write)
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Uart_Ipw_Init/60 Det_ReportError/50 Det_ReportError/50 
Uart_StartSetBuffer/36 (Uart_StartSetBuffer) @06d8de00
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: Uart_SetBuffer/42 
  Calls: Uart_Ipw_SetRxBuffer/58 Uart_Ipw_SetTxBuffer/57 
Uart_StartAsyncSend/35 (Uart_StartAsyncSend) @06d8db60
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: Uart_AsyncSend/46 
  Calls: Uart_Ipw_AsyncSend/56 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartAsyncReceive/34 (Uart_StartAsyncReceive) @06d8d8c0
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: Uart_AsyncReceive/45 
  Calls: Uart_Ipw_AsyncReceive/55 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_StartSyncSend/33 (Uart_StartSyncSend) @06d8d620
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: Uart_SyncSend/43 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncSend/54 Det_ReportError/50 Uart_Ipw_GetTransmitStatus/53 
Uart_StartSyncReceive/32 (Uart_StartSyncReceive) @06d8d380
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: Uart_SyncReceive/44 
  Calls: Det_ReportRuntimeError/52 Uart_Ipw_SyncReceive/51 Det_ReportError/50 Uart_Ipw_GetReceiveStatus/49 
Uart_apConfig/31 (Uart_apConfig) @06cb8318
  Type: variable definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly
  References: 
  Referring: Uart_Init/37 (read)Uart_Init/37 (read)Uart_Init/37 (write)Uart_Init/37 (read)Uart_Init/37 (read)Uart_Deinit/38 (read)Uart_Deinit/38 (write)
  Availability: available
  Varpool flags:
Uart_au32ClockFrequency/30 (Uart_au32ClockFrequency) @06cb8240
  Type: variable definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly
  References: 
  Referring: Uart_Init/37 (write)Uart_SetBaudrate/39 (read)
  Availability: available
  Varpool flags:
Uart_au8DriverStatus/29 (Uart_au8DriverStatus) @06cb81b0
  Type: variable definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly
  References: 
  Referring: Uart_SyncReceive/44 (read)Uart_AsyncReceive/45 (read)Uart_Init/37 (read)Uart_AsyncSend/46 (read)Uart_Init/37 (write)Uart_Deinit/38 (write)Uart_SetBaudrate/39 (read)Uart_GetBaudrate/40 (read)Uart_Abort/41 (read)Uart_SetBuffer/42 (read)Uart_SyncSend/43 (read)Uart_Deinit/38 (read)Uart_GetStatus/47 (read)
  Availability: available
  Varpool flags:
Materializing clones
Materialization Call site updates done.

Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Trivially needed variables: Uart_apConfig Uart_au32ClockFrequency Uart_au8DriverStatus
Removing variables:

Final Symbol table:

Uart_Ipw_AbortReceivingData/65 (Uart_Ipw_AbortReceivingData) @06e2f9a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_AbortSendingData/64 (Uart_Ipw_AbortSendingData) @06e2f8c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_GetBaudrate/63 (Uart_Ipw_GetBaudrate) @06e2f700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_SetBaudrate/62 (Uart_Ipw_SetBaudrate) @06e2f540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_Deinit/61 (Uart_Ipw_Deinit) @06e2f380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_Init/60 (Uart_Ipw_Init) @06e2f1c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_pxPBcfgVariantPredefined/59 (Uart_pxPBcfgVariantPredefined) @06e32000
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Varpool flags: read-only
Uart_Ipw_SetRxBuffer/58 (Uart_Ipw_SetRxBuffer) @06da1ee0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_SetTxBuffer/57 (Uart_Ipw_SetTxBuffer) @06da1e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_AsyncSend/56 (Uart_Ipw_AsyncSend) @06da1c40
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_AsyncReceive/55 (Uart_Ipw_AsyncReceive) @06da1a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_SyncSend/54 (Uart_Ipw_SyncSend) @06da18c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_GetTransmitStatus/53 (Uart_Ipw_GetTransmitStatus) @06da17e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Det_ReportRuntimeError/52 (Det_ReportRuntimeError) @06da1620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_SyncReceive/51 (Uart_Ipw_SyncReceive) @06da1540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Det_ReportError/50 (Det_ReportError) @06da1460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_Ipw_GetReceiveStatus/49 (Uart_Ipw_GetReceiveStatus) @06da1380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: 
  Calls: 
Uart_GetVersionInfo/48 (Uart_GetVersionInfo) @06d95d20
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_GetStatus/47 (Uart_GetStatus) @06d957e0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_AsyncSend/46 (Uart_AsyncSend) @06d952a0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_AsyncReceive/45 (Uart_AsyncReceive) @06d95ee0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_SyncReceive/44 (Uart_SyncReceive) @06d95c40
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_SyncSend/43 (Uart_SyncSend) @06d959a0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_SetBuffer/42 (Uart_SetBuffer) @06d95700
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_Abort/41 (Uart_Abort) @06d95460
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_GetBaudrate/40 (Uart_GetBaudrate) @06d951c0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_SetBaudrate/39 (Uart_SetBaudrate) @06d8dee0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_Deinit/38 (Uart_Deinit) @06d8d9a0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_Init/37 (Uart_Init) @06d8d460
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder asm_written public
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_StartSetBuffer/36 (Uart_StartSetBuffer) @06d8de00
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly asm_written
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_StartAsyncSend/35 (Uart_StartAsyncSend) @06d8db60
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly asm_written
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_StartAsyncReceive/34 (Uart_StartAsyncReceive) @06d8d8c0
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly asm_written
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_StartSyncSend/33 (Uart_StartSyncSend) @06d8d620
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly asm_written
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_StartSyncReceive/32 (Uart_StartSyncReceive) @06d8d380
  Type: function definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly asm_written
  References: 
  Referring: 
  Availability: available
  Function flags:
  Called by: 
  Calls: 
Uart_apConfig/31 (Uart_apConfig) @06cb8318
  Type: variable definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly asm_written
  Aux: @00000001
  References: 
  Referring: 
  Availability: available
  Varpool flags:
Uart_au32ClockFrequency/30 (Uart_au32ClockFrequency) @06cb8240
  Type: variable definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly asm_written
  Aux: @06cb8318
  References: 
  Referring: 
  Availability: available
  Varpool flags:
Uart_au8DriverStatus/29 (Uart_au8DriverStatus) @06cb81b0
  Type: variable definition analyzed
  Visibility: force_output no_reorder prevailing_def_ironly asm_written
  Aux: @06cb8240
  References: 
  Referring: 
  Availability: available
  Varpool flags:
