<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00046.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Uart</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Uart</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T40D2M10I0R0/Uart</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-PRE-COMPILE</IMPLEMENTATION-CONFIG-VARIANT>
          <POST-BUILD-VARIANT-USED>true</POST-BUILD-VARIANT-USED>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>255</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/VendorApiInfix</DEFINITION-REF>
                  <VALUE></VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>GeneralConfiguration</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/DisableUartRuntimeErrorDetect</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/UartCallbackCapability</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/UartDevErrorDetect</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/UartDmaEnable</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/UartEnableUserModeSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/UartMulticoreSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/UartTimeoutDuration</DEFINITION-REF>
                  <VALUE>500000</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/UartTimeoutMethod</DEFINITION-REF>
                  <VALUE>OSIF_COUNTER_DUMMY</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Uart/GeneralConfiguration/UartVersionInfoApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>UartGlobalConfig</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLEXIO_RX</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartChannelId</DEFINITION-REF>
                      <VALUE>3</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartHwUsing</DEFINITION-REF>
                      <VALUE>FLEXIO_IP</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartClockRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuClockSettingConfig_0/McuClockReferencePoint_FLEXIO_CLK</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>FlexioModuleConfiguration</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/DesireBaudrate</DEFINITION-REF>
                          <VALUE>FLEXIO_UART_BAUDRATE_9600</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/FlexioUartInteruptDmaMethod</DEFINITION-REF>
                          <VALUE>FLEXIO_UART_IP_DRIVER_TYPE_INTERRUPTS</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/bitCount</DEFINITION-REF>
                          <VALUE>FLEXIO_UART_IP_8_BITS_PER_CHAR</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/driverDirection</DEFINITION-REF>
                          <VALUE>FLEXIO_UART_IP_DIRECTION_RX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-CHOICE-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/UartHwChannelRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcl/Mcl/MclConfig/FlexioCommon_0/FLEXIO_RX</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLEXIO_TX</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartChannelId</DEFINITION-REF>
                      <VALUE>4</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartHwUsing</DEFINITION-REF>
                      <VALUE>FLEXIO_IP</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartClockRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuClockSettingConfig_0/McuClockReferencePoint_FLEXIO_CLK</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>FlexioModuleConfiguration</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/DesireBaudrate</DEFINITION-REF>
                          <VALUE>FLEXIO_UART_BAUDRATE_9600</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/FlexioUartInteruptDmaMethod</DEFINITION-REF>
                          <VALUE>FLEXIO_UART_IP_DRIVER_TYPE_INTERRUPTS</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/bitCount</DEFINITION-REF>
                          <VALUE>FLEXIO_UART_IP_8_BITS_PER_CHAR</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/driverDirection</DEFINITION-REF>
                          <VALUE>FLEXIO_UART_IP_DIRECTION_TX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-CHOICE-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/FlexioModuleConfiguration/UartHwChannelRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcl/Mcl/MclConfig/FlexioCommon_0/FLEXIO_TX</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>LPUART0_RS232</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartChannelId</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartHwUsing</DEFINITION-REF>
                      <VALUE>LPUART_IP</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartClockRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuClockSettingConfig_0/McuClockReferencePoint_LPUART0_CLK</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DetailModuleConfiguration</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/DesireBaudrate</DEFINITION-REF>
                          <VALUE>LPUART_UART_BAUDRATE_9600</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartCallback</DEFINITION-REF>
                          <VALUE>UART_Callback</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartHwChannel</DEFINITION-REF>
                          <VALUE>LPUART_0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartInteruptDmaMethod</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_USING_DMA</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartParityType</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_PARITY_DISABLED</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartStopBitNumber</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_ONE_STOP_BIT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartWordLength</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_8_BITS_PER_CHAR</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartDmaRxChannelRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcl/Mcl/MclConfig/UART0_RX</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartDmaTxChannelRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcl/Mcl/MclConfig/UART0_TX</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>LPUART1_WIFI</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartChannelId</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartHwUsing</DEFINITION-REF>
                      <VALUE>LPUART_IP</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartClockRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuClockSettingConfig_0/McuClockReferencePoint_LPUART1_CLK</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DetailModuleConfiguration</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/DesireBaudrate</DEFINITION-REF>
                          <VALUE>LPUART_UART_BAUDRATE_115200</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartCallback</DEFINITION-REF>
                          <VALUE>UART_Callback</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartHwChannel</DEFINITION-REF>
                          <VALUE>LPUART_1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartInteruptDmaMethod</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_USING_DMA</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartParityType</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_PARITY_DISABLED</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartStopBitNumber</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_ONE_STOP_BIT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartWordLength</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_8_BITS_PER_CHAR</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartDmaRxChannelRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcl/Mcl/MclConfig/UART1_RX</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartDmaTxChannelRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcl/Mcl/MclConfig/UART1_TX</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>LPUART2_BT</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartChannelId</DEFINITION-REF>
                      <VALUE>2</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartHwUsing</DEFINITION-REF>
                      <VALUE>LPUART_IP</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/UartClockRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuClockSettingConfig_0/McuClockReferencePoint_LPUART2_CLK</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DetailModuleConfiguration</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/DesireBaudrate</DEFINITION-REF>
                          <VALUE>LPUART_UART_BAUDRATE_115200</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartCallback</DEFINITION-REF>
                          <VALUE>UART_Callback</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartHwChannel</DEFINITION-REF>
                          <VALUE>LPUART_2</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartInteruptDmaMethod</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_USING_DMA</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartParityType</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_PARITY_DISABLED</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartStopBitNumber</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_ONE_STOP_BIT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartWordLength</DEFINITION-REF>
                          <VALUE>LPUART_UART_IP_8_BITS_PER_CHAR</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartDmaRxChannelRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcl/Mcl/MclConfig/UART2_RX</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Uart/UartGlobalConfig/UartChannel/DetailModuleConfiguration/UartDmaTxChannelRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcl/Mcl/MclConfig/UART2_TX</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
