
Marking local functions:


Marking externally visible functions: Flexio_3_Uart_Ip_DmaTxCompleteCallback Flexio_3_Uart_Ip_DmaRxCompleteCallback Flexio_2_Uart_Ip_DmaTxCompleteCallback Flexio_2_Uart_Ip_DmaRxCompleteCallback Flexio_1_Uart_Ip_DmaTxCompleteCallback Flexio_1_Uart_Ip_DmaRxCompleteCallback Flexio_0_Uart_Ip_DmaTxCompleteCallback Flexio_0_Uart_Ip_DmaRxCompleteCallback


Marking externally visible variables:


Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Symbol table:

Flexio_Uart_Ip_CompleteSendUsingDma/9 (Flexio_Uart_Ip_CompleteSendUsingDma) @06b0f7e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 
  Calls: 
Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (Flexio_Uart_Ip_CompleteReceiveUsingDma) @06b0f620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 
  Calls: 
Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 (Flexio_3_Uart_Ip_DmaTxCompleteCallback) @06b0f1c0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 
Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 (Flexio_3_Uart_Ip_DmaRxCompleteCallback) @06b0ce00
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 
Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 (Flexio_2_Uart_Ip_DmaTxCompleteCallback) @06b0c8c0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 
Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 (Flexio_2_Uart_Ip_DmaRxCompleteCallback) @06b0c380
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 
Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 (Flexio_1_Uart_Ip_DmaTxCompleteCallback) @06b0cd20
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 
Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 (Flexio_1_Uart_Ip_DmaRxCompleteCallback) @06b0ca80
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 
Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 (Flexio_0_Uart_Ip_DmaTxCompleteCallback) @06b0c7e0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 
Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 (Flexio_0_Uart_Ip_DmaRxCompleteCallback) @06b0c540
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 
Flexio_3_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> :
  Flexio_Uart_Ip_CompleteSendUsingDma (3);
  return;

}


Flexio_3_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> :
  Flexio_Uart_Ip_CompleteReceiveUsingDma (3);
  return;

}


Flexio_2_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> :
  Flexio_Uart_Ip_CompleteSendUsingDma (2);
  return;

}


Flexio_2_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> :
  Flexio_Uart_Ip_CompleteReceiveUsingDma (2);
  return;

}


Flexio_1_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> :
  Flexio_Uart_Ip_CompleteSendUsingDma (1);
  return;

}


Flexio_1_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> :
  Flexio_Uart_Ip_CompleteReceiveUsingDma (1);
  return;

}


Flexio_0_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> :
  Flexio_Uart_Ip_CompleteSendUsingDma (0);
  return;

}


Flexio_0_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> :
  Flexio_Uart_Ip_CompleteReceiveUsingDma (0);
  return;

}


