IPA function summary for Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant


Flattening functions:
Overall time estimate: 104.000000 weighted by profile: 0.000000

Deciding on inlining of small functions.  Starting with size 0.
Enqueueing calls in Flexio_3_Uart_Ip_DmaTxCompleteCallback/7.
Enqueueing calls in Flexio_3_Uart_Ip_DmaRxCompleteCallback/6.
Enqueueing calls in Flexio_2_Uart_Ip_DmaTxCompleteCallback/5.
Enqueueing calls in Flexio_2_Uart_Ip_DmaRxCompleteCallback/4.
Enqueueing calls in Flexio_1_Uart_Ip_DmaTxCompleteCallback/3.
Enqueueing calls in Flexio_1_Uart_Ip_DmaRxCompleteCallback/2.
Enqueueing calls in Flexio_0_Uart_Ip_DmaTxCompleteCallback/1.
Enqueueing calls in Flexio_0_Uart_Ip_DmaRxCompleteCallback/0.

Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:

Deciding on functions to be inlined into all callers and removing useless speculations:
Overall time estimate: 104.000000 weighted by profile: 0.000000

Why inlining failed?
function body not available                       :        8 calls, 8.000000 freq, 0 count
IPA function summary for Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

IPA function summary for Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

Symbol table:

Flexio_Uart_Ip_CompleteSendUsingDma/9 (Flexio_Uart_Ip_CompleteSendUsingDma) @05df57e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 (1073741824 (estimated locally),1.00 per call) Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 (1073741824 (estimated locally),1.00 per call) Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 (1073741824 (estimated locally),1.00 per call) Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (Flexio_Uart_Ip_CompleteReceiveUsingDma) @05df5620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 (1073741824 (estimated locally),1.00 per call) Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 (1073741824 (estimated locally),1.00 per call) Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 (1073741824 (estimated locally),1.00 per call) Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 (Flexio_3_Uart_Ip_DmaTxCompleteCallback) @05df51c0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 (1073741824 (estimated locally),1.00 per call) 
Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 (Flexio_3_Uart_Ip_DmaRxCompleteCallback) @05df1e00
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (1073741824 (estimated locally),1.00 per call) 
Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 (Flexio_2_Uart_Ip_DmaTxCompleteCallback) @05df18c0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 (1073741824 (estimated locally),1.00 per call) 
Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 (Flexio_2_Uart_Ip_DmaRxCompleteCallback) @05df1380
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (1073741824 (estimated locally),1.00 per call) 
Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 (Flexio_1_Uart_Ip_DmaTxCompleteCallback) @05df1d20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 (1073741824 (estimated locally),1.00 per call) 
Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 (Flexio_1_Uart_Ip_DmaRxCompleteCallback) @05df1a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (1073741824 (estimated locally),1.00 per call) 
Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 (Flexio_0_Uart_Ip_DmaTxCompleteCallback) @05df17e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 (1073741824 (estimated locally),1.00 per call) 
Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 (Flexio_0_Uart_Ip_DmaRxCompleteCallback) @05df1540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (1073741824 (estimated locally),1.00 per call) 

;; Function Flexio_0_Uart_Ip_DmaRxCompleteCallback (Flexio_0_Uart_Ip_DmaRxCompleteCallback, funcdef_no=0, decl_uid=5694, cgraph_uid=1, symbol_order=0)

Flexio_0_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (0);
  return;

}



;; Function Flexio_0_Uart_Ip_DmaTxCompleteCallback (Flexio_0_Uart_Ip_DmaTxCompleteCallback, funcdef_no=1, decl_uid=5696, cgraph_uid=2, symbol_order=1)

Flexio_0_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (0);
  return;

}



;; Function Flexio_1_Uart_Ip_DmaRxCompleteCallback (Flexio_1_Uart_Ip_DmaRxCompleteCallback, funcdef_no=2, decl_uid=5698, cgraph_uid=3, symbol_order=2)

Flexio_1_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (1);
  return;

}



;; Function Flexio_1_Uart_Ip_DmaTxCompleteCallback (Flexio_1_Uart_Ip_DmaTxCompleteCallback, funcdef_no=3, decl_uid=5700, cgraph_uid=4, symbol_order=3)

Flexio_1_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (1);
  return;

}



;; Function Flexio_2_Uart_Ip_DmaRxCompleteCallback (Flexio_2_Uart_Ip_DmaRxCompleteCallback, funcdef_no=4, decl_uid=5702, cgraph_uid=5, symbol_order=4)

Flexio_2_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (2);
  return;

}



;; Function Flexio_2_Uart_Ip_DmaTxCompleteCallback (Flexio_2_Uart_Ip_DmaTxCompleteCallback, funcdef_no=5, decl_uid=5704, cgraph_uid=6, symbol_order=5)

Flexio_2_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (2);
  return;

}



;; Function Flexio_3_Uart_Ip_DmaRxCompleteCallback (Flexio_3_Uart_Ip_DmaRxCompleteCallback, funcdef_no=6, decl_uid=5706, cgraph_uid=7, symbol_order=6)

Flexio_3_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (3);
  return;

}



;; Function Flexio_3_Uart_Ip_DmaTxCompleteCallback (Flexio_3_Uart_Ip_DmaTxCompleteCallback, funcdef_no=7, decl_uid=5708, cgraph_uid=8, symbol_order=7)

Flexio_3_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (3);
  return;

}


