callgraph:

Uart_Ipw_LpuartCallback/32 (Uart_Ipw_LpuartCallback) @05f81540
  Type: function
  Visibility: external public
  Address is taken.
  References: 
  Referring: Lpuart_Uart_Ip_xHwConfigPB_0_VS_0/29 (addr)Lpuart_Uart_Ip_xHwConfigPB_1_VS_0/30 (addr)Lpuart_Uart_Ip_xHwConfigPB_2_VS_0/31 (addr)
  Availability: not_available
  Function flags: optimize_size
  Called by: 
  Calls: 


 ordered call graph: reduced for nothrow



MALLOC LATTICE Initial:


MALLOC LATTICE after propagation:
callgraph:

Uart_Ipw_LpuartCallback/32 (Uart_Ipw_LpuartCallback) @05f81540
  Type: function
  Visibility: external public
  Address is taken.
  References: 
  Referring: Lpuart_Uart_Ip_xHwConfigPB_0_VS_0/29 (addr)Lpuart_Uart_Ip_xHwConfigPB_1_VS_0/30 (addr)Lpuart_Uart_Ip_xHwConfigPB_2_VS_0/31 (addr)
  Availability: not_available
  Function flags: optimize_size
  Called by: 
  Calls: 


 ordered call graph: reduced

