<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00046.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Can</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Can</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/Can_TS_T40D2M10I0R0/Can</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-PRE-COMPILE</IMPLEMENTATION-CONFIG-VARIANT>
          <POST-BUILD-VARIANT-USED>true</POST-BUILD-VARIANT-USED>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CanConfigSet</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>CanController_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanAutoBusOffRecovery</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanBusoffProcessing</DEFINITION-REF>
                      <VALUE>POLLING</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanClockFromBus</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerActivation</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaseAddress</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerEdgeFilter</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerFdISO</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerId</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerPrExcEn</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanFDErrorNotification</DEFINITION-REF>
                      <VALUE>NULL_PTR</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanHwChannel</DEFINITION-REF>
                      <VALUE>FLEXCAN_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanLoopBackMode</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxProcessing</DEFINITION-REF>
                      <VALUE>POLLING</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanTrippleSamplingEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanTxProcessing</DEFINITION-REF>
                      <VALUE>POLLING</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanWakeupFunctionalityAPI</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanWakeupProcessing</DEFINITION-REF>
                      <VALUE>POLLING</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanWakeupSupport</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerDefaultBaudrate</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Can/Can/CanConfigSet/CanController_0/CanControllerBaudrateConfig_250K</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanCpuClockRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuClockSettingConfig_0/McuClockReferencePoint_CAN</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanCpuClockRefAlternate</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanControllerBaudrateConfig_250K</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanAdvancedSetting</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanBaudrateTypeSuport</DEFINITION-REF>
                          <VALUE>NORMAL_CBT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanBusLength</DEFINITION-REF>
                          <VALUE>40</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerBaudRate</DEFINITION-REF>
                          <VALUE>250.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerBaudRateConfigID</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerPrescaller</DEFINITION-REF>
                          <VALUE>12</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerPrescallerAlternate</DEFINITION-REF>
                          <VALUE>10</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerPropSeg</DEFINITION-REF>
                          <VALUE>5</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerSeg1</DEFINITION-REF>
                          <VALUE>5</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerSeg2</DEFINITION-REF>
                          <VALUE>6</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerSyncJumpWidth</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanControllerSyncSeg</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanPropDelayTranceiver</DEFINITION-REF>
                          <VALUE>150.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanControllerBaudrateConfig/CanTxArbitrationStartDelay</DEFINITION-REF>
                          <VALUE>12</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanRxFiFo</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>CanRxFiFo</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo</DEFINITION-REF>
                          <PARAMETER-VALUES>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanFiFoDmaErrorNotif</DEFINITION-REF>
                              <VALUE>NULL_PTR</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanFiFoOverflowNotif</DEFINITION-REF>
                              <VALUE>NULL_PTR</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanFiFoWarnNotif</DEFINITION-REF>
                              <VALUE>NULL_PTR</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanIdAcceptanceMode</DEFINITION-REF>
                              <VALUE>FORMAT_A</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanLegacyFIFOGlobalMask0</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanLegacyFIFOGlobalMask1</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanLegacyFIFOGlobalMask2</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanLegacyFIFOGlobalMask3</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanController/CanRxFiFo/CanLegacyFiFo/CanLegacyFiFoDmaEnable</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                          </PARAMETER-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>Can0HardwareObject_RX</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHandleType</DEFINITION-REF>
                      <VALUE>BASIC</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwObjectCount</DEFINITION-REF>
                      <VALUE>6</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanIdType</DEFINITION-REF>
                      <VALUE>EXTENDED</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanObjectId</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanObjectType</DEFINITION-REF>
                      <VALUE>RECEIVE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanTimeStampEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanControllerRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Can/Can/CanConfigSet/CanController_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanMainFunctionRWPeriodRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Can/Can/CanGeneral/CanMainFunctionRWPeriods_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanHwFilter_0</SHORT-NAME>
                      <INDEX>0</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterCode</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterMask</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanHwFilter_1</SHORT-NAME>
                      <INDEX>1</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterCode</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterMask</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanHwFilter_2</SHORT-NAME>
                      <INDEX>2</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterCode</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterMask</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanHwFilter_3</SHORT-NAME>
                      <INDEX>3</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterCode</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterMask</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanHwFilter_4</SHORT-NAME>
                      <INDEX>4</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterCode</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterMask</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanHwFilter_5</SHORT-NAME>
                      <INDEX>5</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterCode</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterMask</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanHwFilter_6</SHORT-NAME>
                      <INDEX>6</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterCode</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterMask</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanHwFilter_7</SHORT-NAME>
                      <INDEX>7</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterCode</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwFilter/CanHwFilterMask</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>Can0HardwareObject_TX</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHandleType</DEFINITION-REF>
                      <VALUE>BASIC</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanHwObjectCount</DEFINITION-REF>
                      <VALUE>10</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanIdType</DEFINITION-REF>
                      <VALUE>EXTENDED</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanObjectId</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanObjectType</DEFINITION-REF>
                      <VALUE>TRANSMIT</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanTimeStampEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanControllerRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Can/Can/CanConfigSet/CanController_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanHardwareObject/CanMainFunctionRWPeriodRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Can/Can/CanGeneral/CanMainFunctionRWPeriods_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>CanIcom</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom</DEFINITION-REF>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>CanIcomConfig_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomConfigId</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeOnBusOff</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>CanIcomWakeupCauses</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeupCauses</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>CanIcomRxMessage_0</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeupCauses/CanIcomRxMessage</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeupCauses/CanIcomRxMessage/CanIcomCounterValue</DEFINITION-REF>
                                  <VALUE>2</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeupCauses/CanIcomRxMessage/CanIcomIdOperation</DEFINITION-REF>
                                  <VALUE>GREATER_MINNUM</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeupCauses/CanIcomRxMessage/CanIcomMessageId</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeupCauses/CanIcomRxMessage/CanIcomMessageIdType</DEFINITION-REF>
                                  <VALUE>EXTENDED</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeupCauses/CanIcomRxMessage/CanIcomPayloadLengthError</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanConfigSet/CanIcom/CanIcomConfig/CanIcomWakeupCauses/CanIcomRxMessage/CanPayloadFilter</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CanGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanApiEnableMbAbort</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanDevErrorDetect</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanEnableDualClockMode</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanEnableUserModeSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanIndex</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanMBCountExtensionSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanMainFunctionBusoffPeriod</DEFINITION-REF>
                  <VALUE>0.001</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanMainFunctionModePeriod</DEFINITION-REF>
                  <VALUE>0.001</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanMulticoreSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanMultiplexedTransmission</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanPublicIcomSupport</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanSetBaudrateApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanTimeoutDuration</DEFINITION-REF>
                  <VALUE>1.0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanTimeoutMethod</DEFINITION-REF>
                  <VALUE>OSIF_COUNTER_DUMMY</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanVersionInfoApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
              <REFERENCE-VALUES>
                <ECUC-REFERENCE-VALUE>
                  <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanSupportTTCANRef</DEFINITION-REF>
                </ECUC-REFERENCE-VALUE>
              </REFERENCE-VALUES>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>CanIcomGeneral</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanIcomGeneral</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanIcomGeneral/CanIcomLevel</DEFINITION-REF>
                      <VALUE>CAN_ICOM_LEVEL_ONE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanIcomGeneral/CanIcomVariant</DEFINITION-REF>
                      <VALUE>CAN_ICOM_VARIANT_NONE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>CanMainFunctionRWPeriods_0</SHORT-NAME>
                  <INDEX>0</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanMainFunctionRWPeriods</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CanGeneral/CanMainFunctionRWPeriods/CanMainFunctionPeriod</DEFINITION-REF>
                      <VALUE>0.001</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>80</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/VendorApiInfix</DEFINITION-REF>
                  <VALUE></VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/Can_TS_T40D2M10I0R0/Can/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
