Callgraph clone;Lpuart_Uart_Ip_ClearStatusFlag;22;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20;Lpuart_Uart_Ip_ClearStatusFlag.part.0;83;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20;part
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_StartSendDataUsingInt;54;../RTD/src/Lpuart_Uart_Ip.c;1431;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;221;20;Lpuart_Uart_Ip_StartSendDataUsingInt;54;../RTD/src/Lpuart_Uart_Ip.c;1431;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_FlushRxBuffer;28;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;720;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_Putchar;15;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;480;20;Lpuart_Uart_Ip_PutData;63;../RTD/src/Lpuart_Uart_Ip.c;2015;13;inlining to
Callgraph removal;Lpuart_Uart_Ip_Putchar;15;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;480;20
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_TxEmptyIrqHandler;51;../RTD/src/Lpuart_Uart_Ip.c;1250;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_TxEmptyIrqHandler;51;../RTD/src/Lpuart_Uart_Ip.c;1250;13;inlining to
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;93;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph clone;Lpuart_Uart_Ip_Getchar;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21;Lpuart_Uart_Ip_GetData;64;../RTD/src/Lpuart_Uart_Ip.c;2074;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;221;20;Lpuart_Uart_Ip_CompleteSendDataUsingInt;56;../RTD/src/Lpuart_Uart_Ip.c;1530;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_CompleteSendDataUsingInt;56;../RTD/src/Lpuart_Uart_Ip.c;1530;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteSendDataUsingInt;56;../RTD/src/Lpuart_Uart_Ip.c;1530;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteSendDataUsingInt;56;../RTD/src/Lpuart_Uart_Ip.c;1530;13;inlining to
Callgraph removal;Lpuart_Uart_Ip_GetStatusFlag;97;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23
Callgraph clone;Lpuart_Uart_Ip_ClearStatusFlagWithMask;23;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;655;20;Lpuart_Uart_Ip_StartGetData;41;../RTD/src/Lpuart_Uart_Ip.c;709;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20;Lpuart_Uart_Ip_StartGetData;41;../RTD/src/Lpuart_Uart_Ip.c;709;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_StartGetData;41;../RTD/src/Lpuart_Uart_Ip.c;709;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_StartGetData;41;../RTD/src/Lpuart_Uart_Ip.c;709;13;inlining to
Callgraph removal;Lpuart_Uart_Ip_GetStatusFlag;101;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23
Callgraph removal;Lpuart_Uart_Ip_ClearStatusFlagWithMask;23;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;655;20
Callgraph clone;Lpuart_Uart_Ip_Getchar;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;60;../RTD/src/Lpuart_Uart_Ip.c;1814;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;60;../RTD/src/Lpuart_Uart_Ip.c;1814;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;60;../RTD/src/Lpuart_Uart_Ip.c;1814;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;60;../RTD/src/Lpuart_Uart_Ip.c;1814;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;60;../RTD/src/Lpuart_Uart_Ip.c;1814;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;60;../RTD/src/Lpuart_Uart_Ip.c;1814;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;60;../RTD/src/Lpuart_Uart_Ip.c;1814;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;60;../RTD/src/Lpuart_Uart_Ip.c;1814;13;inlining to
Callgraph removal;Lpuart_Uart_Ip_GetStatusFlag;105;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23
Callgraph removal;Lpuart_Uart_Ip_SetReceiverCmd;104;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20
Callgraph clone;Lpuart_Uart_Ip_SetTxDmaCmd;13;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;451;20;Lpuart_Uart_Ip_StartSendDataUsingDma;55;../RTD/src/Lpuart_Uart_Ip.c;1464;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;221;20;Lpuart_Uart_Ip_StartSendDataUsingDma;55;../RTD/src/Lpuart_Uart_Ip.c;1464;34;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_StartSendDataUsingDma;55;../RTD/src/Lpuart_Uart_Ip.c;1464;34;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_StartSendDataUsingDma;55;../RTD/src/Lpuart_Uart_Ip.c;1464;34;inlining to
Callgraph removal;Lpuart_Uart_Ip_SetTxDmaCmd;111;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;451;20
Callgraph removal;DevAssert;113;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph clone;Lpuart_Uart_Ip_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20;Lpuart_Uart_Ip_StartReceiveDataUsingDma;59;../RTD/src/Lpuart_Uart_Ip.c;1742;34;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_StartReceiveDataUsingDma;59;../RTD/src/Lpuart_Uart_Ip.c;1742;34;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_StartReceiveDataUsingDma;59;../RTD/src/Lpuart_Uart_Ip.c;1742;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_FlushRxBuffer;28;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;720;20;Lpuart_Uart_Ip_StartReceiveDataUsingDma;59;../RTD/src/Lpuart_Uart_Ip.c;1742;34;inlining to
Callgraph removal;DevAssert;116;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_FlushRxBuffer;118;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;720;20
Callgraph clone;Lpuart_Uart_Ip_EnableBothEdgeSamplingCmd;7;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;316;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_Hw_Init;0;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;200;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph removal;DevAssert;121;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_Hw_Init;0;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;200;20
Callgraph removal;Lpuart_Uart_Ip_EnableBothEdgeSamplingCmd;119;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;316;20
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_Deinit;35;../RTD/src/Lpuart_Uart_Ip.c;327;6;inlining to
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;127;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;128;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;130;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph clone;Lpuart_Uart_Ip_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;221;20;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;221;20;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SyncSend;36;../RTD/src/Lpuart_Uart_Ip.c;370;27;inlining to
Callgraph removal;DevAssert;142;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;DevAssert;143;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;140;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;37;../RTD/src/Lpuart_Uart_Ip.c;453;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;37;../RTD/src/Lpuart_Uart_Ip.c;453;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;37;../RTD/src/Lpuart_Uart_Ip.c;453;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;37;../RTD/src/Lpuart_Uart_Ip.c;453;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;37;../RTD/src/Lpuart_Uart_Ip.c;453;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;37;../RTD/src/Lpuart_Uart_Ip.c;453;27;inlining to
Callgraph removal;DevAssert;149;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_GetTransmitStatus;38;../RTD/src/Lpuart_Uart_Ip.c;515;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_GetTransmitStatus;38;../RTD/src/Lpuart_Uart_Ip.c;515;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_GetTransmitStatus;38;../RTD/src/Lpuart_Uart_Ip.c;515;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_Getchar;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph removal;DevAssert;159;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;DevAssert;162;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;42;../RTD/src/Lpuart_Uart_Ip.c;774;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;42;../RTD/src/Lpuart_Uart_Ip.c;774;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;42;../RTD/src/Lpuart_Uart_Ip.c;774;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;42;../RTD/src/Lpuart_Uart_Ip.c;774;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;42;../RTD/src/Lpuart_Uart_Ip.c;774;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;42;../RTD/src/Lpuart_Uart_Ip.c;774;27;inlining to
Callgraph removal;DevAssert;167;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_GetReceiveStatus;43;../RTD/src/Lpuart_Uart_Ip.c;836;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_GetReceiveStatus;43;../RTD/src/Lpuart_Uart_Ip.c;836;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_GetReceiveStatus;43;../RTD/src/Lpuart_Uart_Ip.c;836;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_EnableBothEdgeSamplingCmd;7;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;316;20;Lpuart_Uart_Ip_SetBaudRate;45;../RTD/src/Lpuart_Uart_Ip.c;950;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetBaudRate;45;../RTD/src/Lpuart_Uart_Ip.c;950;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetBaudRate;45;../RTD/src/Lpuart_Uart_Ip.c;950;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetBaudRate;45;../RTD/src/Lpuart_Uart_Ip.c;950;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetBaudRate;45;../RTD/src/Lpuart_Uart_Ip.c;950;27;inlining to
Callgraph removal;DevAssert;175;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_EnableBothEdgeSamplingCmd;7;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;316;20
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_GetBaudRate;46;../RTD/src/Lpuart_Uart_Ip.c;1060;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_GetBaudRate;46;../RTD/src/Lpuart_Uart_Ip.c;1060;6;inlining to
Callgraph removal;DevAssert;176;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetTxBuffer;47;../RTD/src/Lpuart_Uart_Ip.c;1081;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetTxBuffer;47;../RTD/src/Lpuart_Uart_Ip.c;1081;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetTxBuffer;47;../RTD/src/Lpuart_Uart_Ip.c;1081;27;inlining to
Callgraph removal;DevAssert;179;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetRxBuffer;48;../RTD/src/Lpuart_Uart_Ip.c;1108;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetRxBuffer;48;../RTD/src/Lpuart_Uart_Ip.c;1108;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_SetRxBuffer;48;../RTD/src/Lpuart_Uart_Ip.c;1108;27;inlining to
Callgraph removal;DevAssert;182;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph clone;Lpuart_Uart_Ip_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;221;20;Lpuart_Uart_Ip_CompleteSendUsingDma;57;../RTD/src/Lpuart_Uart_Ip.c;1584;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_CompleteSendUsingDma;57;../RTD/src/Lpuart_Uart_Ip.c;1584;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetTxDmaCmd;13;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;451;20;Lpuart_Uart_Ip_CompleteSendUsingDma;57;../RTD/src/Lpuart_Uart_Ip.c;1584;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_CompleteSendUsingDma;57;../RTD/src/Lpuart_Uart_Ip.c;1584;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_CompleteSendUsingDma;57;../RTD/src/Lpuart_Uart_Ip.c;1584;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_CompleteSendUsingDma;57;../RTD/src/Lpuart_Uart_Ip.c;1584;6;inlining to
Callgraph removal;DevAssert;187;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;DevAssert;185;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_SetTxDmaCmd;13;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;451;20
Callgraph removal;Lpuart_Uart_Ip_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;221;20
Callgraph clone;Lpuart_Uart_Ip_FlushTxBuffer;27;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;708;20;Lpuart_Uart_Ip_AbortSendingData;39;../RTD/src/Lpuart_Uart_Ip.c;570;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AbortSendingData;39;../RTD/src/Lpuart_Uart_Ip.c;570;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AbortSendingData;39;../RTD/src/Lpuart_Uart_Ip.c;570;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AbortSendingData;39;../RTD/src/Lpuart_Uart_Ip.c;570;27;inlining to
Callgraph removal;DevAssert;188;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;DevAssert;190;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_FlushTxBuffer;27;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;708;20
Callgraph clone;Lpuart_Uart_Ip_Getchar;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph removal;DevAssert;194;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_GetStatusFlag;192;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23
Callgraph removal;Lpuart_Uart_Ip_Getchar;191;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21
Callgraph removal;Lpuart_Uart_Ip_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;236;20
Callgraph clone;Lpuart_Uart_Ip_FlushRxBuffer;28;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;720;20;Lpuart_Uart_Ip_AbortReceivingData;44;../RTD/src/Lpuart_Uart_Ip.c;889;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AbortReceivingData;44;../RTD/src/Lpuart_Uart_Ip.c;889;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AbortReceivingData;44;../RTD/src/Lpuart_Uart_Ip.c;889;27;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_AbortReceivingData;44;../RTD/src/Lpuart_Uart_Ip.c;889;27;inlining to
Callgraph removal;DevAssert;196;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;DevAssert;197;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;DevAssert;198;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_FlushRxBuffer;28;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;720;20
Callgraph clone;Lpuart_Uart_Ip_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearStatusFlag;22;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearStatusFlag;22;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearStatusFlag;22;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearStatusFlag;22;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph removal;Lpuart_Uart_Ip_ClearStatusFlag;22;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20
Callgraph removal;Lpuart_Uart_Ip_GetIntMode;206;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23
Callgraph removal;Lpuart_Uart_Ip_ClearStatusFlag;207;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20
Callgraph removal;Lpuart_Uart_Ip_GetIntMode;203;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23
Callgraph removal;Lpuart_Uart_Ip_GetStatusFlag;202;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23
Callgraph removal;Lpuart_Uart_Ip_GetIntMode;199;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23
Callgraph removal;Lpuart_Uart_Ip_ClearStatusFlag;200;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20
Callgraph clone;Lpuart_Uart_Ip_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_Getchar;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_Getchar;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph removal;DevAssert;29;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include/devassert.h;65;20
Callgraph removal;Lpuart_Uart_Ip_Getchar;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21
Callgraph removal;Lpuart_Uart_Ip_GetStatusFlag;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23
Callgraph removal;Lpuart_Uart_Ip_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23
Callgraph removal;Lpuart_Uart_Ip_Getchar;215;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;548;21
Callgraph removal;Lpuart_Uart_Ip_GetIntMode;213;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23
Callgraph removal;Lpuart_Uart_Ip_GetStatusFlag;212;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;605;23
Callgraph removal;Lpuart_Uart_Ip_GetIntMode;211;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;434;23
Callgraph removal;__builtin_unreachable;201;<built-in>;0;0
Callgraph clone;Lpuart_Uart_Ip_CheckTimeout;26;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;694;23;Lpuart_Uart_Ip_CheckTimeout.constprop.0;216;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;694;23;constprop
Callgraph clone;Lpuart_Uart_Ip_StartTimeout;25;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;682;20;Lpuart_Uart_Ip_StartTimeout.constprop.0;217;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;682;20;constprop
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_SetupIntDmaMode;62;../RTD/src/Lpuart_Uart_Ip.c;1991;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_SetupIntDmaMode;62;../RTD/src/Lpuart_Uart_Ip.c;1991;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_SetupIntDmaMode;62;../RTD/src/Lpuart_Uart_Ip.c;1991;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_SetupIntDmaMode;62;../RTD/src/Lpuart_Uart_Ip.c;1991;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearErrorFlags;24;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;667;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetRxDmaCmd;14;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;465;20;Lpuart_Uart_Ip_SetupIntDmaMode;62;../RTD/src/Lpuart_Uart_Ip.c;1991;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearErrorFlags;24;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;667;20;Lpuart_Uart_Ip_StartReceiveDataUsingDma;59;../RTD/src/Lpuart_Uart_Ip.c;1742;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_Getchar9;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;561;22;Lpuart_Uart_Ip_GetData;64;../RTD/src/Lpuart_Uart_Ip.c;2074;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearErrorFlags;24;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;667;20;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearStatusFlag.part.0;83;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_ClearErrorFlags;24;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;667;20;Lpuart_Uart_Ip_AbortReceivingData;44;../RTD/src/Lpuart_Uart_Ip.c;889;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_Getchar10;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;581;22;Lpuart_Uart_Ip_GetData;64;../RTD/src/Lpuart_Uart_Ip.c;2074;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_Putchar9;16;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;495;20;Lpuart_Uart_Ip_PutData;63;../RTD/src/Lpuart_Uart_Ip.c;2015;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_Putchar10;17;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;519;20;Lpuart_Uart_Ip_PutData;63;../RTD/src/Lpuart_Uart_Ip.c;2015;13;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetBaudRateDivisor;3;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;250;20;Lpuart_Uart_Ip_SetBaudRate;45;../RTD/src/Lpuart_Uart_Ip.c;950;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetOversamplingRatio;5;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;283;20;Lpuart_Uart_Ip_SetBaudRate;45;../RTD/src/Lpuart_Uart_Ip.c;950;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetBaudRateDivisor;3;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;250;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetStopBitCount;10;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;403;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetOversamplingRatio;5;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;283;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetParityMode;9;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;386;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetBitCountPerChar;8;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;333;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetBitCountPerChar;8;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;333;20;Lpuart_Uart_Ip_Init;34;../RTD/src/Lpuart_Uart_Ip.c;243;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_RxIrqHandler;50;../RTD/src/Lpuart_Uart_Ip.c;1208;13;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_TxCompleteIrqHandler;52;../RTD/src/Lpuart_Uart_Ip.c;1288;13;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_TxEmptyIrqHandler;51;../RTD/src/Lpuart_Uart_Ip.c;1250;13;Lpuart_Uart_Ip_IrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1134;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_StartSendDataUsingInt;54;../RTD/src/Lpuart_Uart_Ip.c;1431;34;Lpuart_Uart_Ip_AsyncSend;37;../RTD/src/Lpuart_Uart_Ip.c;453;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_StartGetData;41;../RTD/src/Lpuart_Uart_Ip.c;709;13;Lpuart_Uart_Ip_SyncReceive;40;../RTD/src/Lpuart_Uart_Ip.c;626;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetupIntDmaMode;62;../RTD/src/Lpuart_Uart_Ip.c;1991;13;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;219;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;220;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetIntMode;218;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetRxDmaCmd;14;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;465;20;Lpuart_Uart_Ip_CompleteReceiveUsingDma;61;../RTD/src/Lpuart_Uart_Ip.c;1874;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_SetupIntDmaMode;62;../RTD/src/Lpuart_Uart_Ip.c;1991;13;Lpuart_Uart_Ip_StartReceiveDataUsingDma;59;../RTD/src/Lpuart_Uart_Ip.c;1742;34;inlining to
Callgraph clone;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34;Lpuart_Uart_Ip_AsyncReceive;42;../RTD/src/Lpuart_Uart_Ip.c;774;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_StartSendDataUsingDma;55;../RTD/src/Lpuart_Uart_Ip.c;1464;34;Lpuart_Uart_Ip_AsyncSend;37;../RTD/src/Lpuart_Uart_Ip.c;453;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_StartReceiveDataUsingDma;59;../RTD/src/Lpuart_Uart_Ip.c;1742;34;Lpuart_Uart_Ip_AsyncReceive;42;../RTD/src/Lpuart_Uart_Ip.c;774;27;inlining to
Callgraph removal;Lpuart_Uart_Ip_CheckTimeout;26;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;694;23
Callgraph removal;Lpuart_Uart_Ip_StartTimeout;25;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;682;20
Callgraph removal;Lpuart_Uart_Ip_Putchar9;16;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;495;20
Callgraph removal;Lpuart_Uart_Ip_Putchar10;17;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;519;20
Callgraph removal;Lpuart_Uart_Ip_Getchar9;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;561;22
Callgraph removal;Lpuart_Uart_Ip_Getchar10;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;581;22
Callgraph removal;Lpuart_Uart_Ip_SetBaudRateDivisor;3;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;250;20
Callgraph removal;Lpuart_Uart_Ip_SetOversamplingRatio;5;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;283;20
Callgraph removal;Lpuart_Uart_Ip_SetBitCountPerChar;8;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;333;20
Callgraph removal;Lpuart_Uart_Ip_SetStopBitCount;10;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;403;20
Callgraph removal;Lpuart_Uart_Ip_SetParityMode;9;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;386;20
Callgraph removal;Lpuart_Uart_Ip_StartSendDataUsingInt;54;../RTD/src/Lpuart_Uart_Ip.c;1431;34
Callgraph removal;Lpuart_Uart_Ip_StartSendDataUsingDma;55;../RTD/src/Lpuart_Uart_Ip.c;1464;34
Callgraph removal;Lpuart_Uart_Ip_StartGetData;41;../RTD/src/Lpuart_Uart_Ip.c;709;13
Callgraph removal;Lpuart_Uart_Ip_StartReceiveDataUsingInt;58;../RTD/src/Lpuart_Uart_Ip.c;1696;34
Callgraph removal;Lpuart_Uart_Ip_ClearErrorFlags;221;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;667;20
Callgraph removal;Lpuart_Uart_Ip_StartReceiveDataUsingDma;59;../RTD/src/Lpuart_Uart_Ip.c;1742;34
Callgraph removal;Lpuart_Uart_Ip_ClearErrorFlags;222;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;667;20
Callgraph removal;Lpuart_Uart_Ip_SetupIntDmaMode;62;../RTD/src/Lpuart_Uart_Ip.c;1991;13
Callgraph removal;Lpuart_Uart_Ip_SetRxDmaCmd;14;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;465;20
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;218;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;220;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;219;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph removal;Lpuart_Uart_Ip_SetBaudRateDivisor;224;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;250;20
Callgraph removal;Lpuart_Uart_Ip_SetOversamplingRatio;225;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;283;20
Callgraph removal;Lpuart_Uart_Ip_SetupIntDmaMode;227;../RTD/src/Lpuart_Uart_Ip.c;1991;13
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;230;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph removal;Lpuart_Uart_Ip_SetIntMode;228;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;419;20
Callgraph removal;Lpuart_Uart_Ip_ClearErrorFlags;24;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;667;20
Callgraph removal;Lpuart_Uart_Ip_ClearErrorFlags;223;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;667;20
Callgraph removal;Lpuart_Uart_Ip_ErrIrqHandler;53;../RTD/src/Lpuart_Uart_Ip.c;1318;13
Callgraph removal;Lpuart_Uart_Ip_ClearStatusFlag.part.0;83;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;621;20
Callgraph removal;Lpuart_Uart_Ip_RxIrqHandler;50;../RTD/src/Lpuart_Uart_Ip.c;1208;13
Callgraph removal;Lpuart_Uart_Ip_TxEmptyIrqHandler;51;../RTD/src/Lpuart_Uart_Ip.c;1250;13
Callgraph removal;Lpuart_Uart_Ip_TxCompleteIrqHandler;52;../RTD/src/Lpuart_Uart_Ip.c;1288;13
