Can_ErrorIrqCallback (uint8 u8Instance, Flexcan_Ip_EventType event, uint32 u32ErrStatus, const struct Flexcan_Ip_StateType * driverState)
{
  <bb 2> :
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (event_2(D) == 9)
    goto <bb 3>; [INV]
  else
    goto <bb 4>; [INV]

  <bb 3> :
<L0>:
  # DEBUG BEGIN_STMT
  Can_ProcessBusOffInterrupt (u8Instance_4(D));
  # DEBUG BEGIN_STMT

  <bb 4> :
  return;

}


Can_CommonIrqCallback (uint8 u8Instance, Flexcan_Ip_EventType event, uint32 u32buffIdx, const struct Flexcan_Ip_StateType * driverState)
{
  <bb 2> :
  # DEBUG BEGIN_STMT
  if (event_2(D) == 6)
    goto <bb 3>; [INV]
  else
    goto <bb 4>; [INV]

  <bb 3> :
  # DEBUG BEGIN_STMT
  Can_ProcessPNInterrupt (u8Instance_4(D));

  <bb 4> :
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return;

}


