
Marking local functions:


Marking externally visible functions: Can_ErrorIrqCallback Can_CommonIrqCallback


Marking externally visible variables:

Clearing variable flags:

Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Symbol table:

Can_ProcessBusOffInterrupt/3 (Can_ProcessBusOffInterrupt) @063917e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Can_ErrorIrqCallback/1 (217325345 (estimated locally),0.20 per call) 
  Calls: 
Can_ProcessPNInterrupt/2 (Can_ProcessPNInterrupt) @06391620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Can_CommonIrqCallback/0 (217325345 (estimated locally),0.20 per call) 
  Calls: 
Can_ErrorIrqCallback/1 (Can_ErrorIrqCallback) @063911c0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Can_ProcessBusOffInterrupt/3 (217325345 (estimated locally),0.20 per call) 
Can_CommonIrqCallback/0 (Can_CommonIrqCallback) @0638aee0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Can_ProcessPNInterrupt/2 (217325345 (estimated locally),0.20 per call) 
Can_ErrorIrqCallback (uint8 u8Instance, Flexcan_Ip_EventType event, uint32 u32ErrStatus, const struct Flexcan_Ip_StateType * driverState)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (event_2(D) == 9)
    goto <bb 3>; [20.24%]
  else
    goto <bb 4>; [79.76%]

  <bb 3> [local count: 217325345]:
<L0>:
  # DEBUG BEGIN_STMT
  Can_ProcessBusOffInterrupt (u8Instance_4(D));
  # DEBUG BEGIN_STMT

  <bb 4> [local count: 1073741824]:
  return;

}


Can_CommonIrqCallback (uint8 u8Instance, Flexcan_Ip_EventType event, uint32 u32buffIdx, const struct Flexcan_Ip_StateType * driverState)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (event_2(D) == 6)
    goto <bb 3>; [20.24%]
  else
    goto <bb 4>; [79.76%]

  <bb 3> [local count: 217325345]:
  # DEBUG BEGIN_STMT
  Can_ProcessPNInterrupt (u8Instance_4(D));

  <bb 4> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return;

}


