Parsed function:Lpuart_2_Uart_Ip_DmaTxCompleteCallback
Parsed function:Lpuart_2_Uart_Ip_DmaRxCompleteCallback
Parsed function:Lpuart_1_Uart_Ip_DmaTxCompleteCallback
Parsed function:Lpuart_1_Uart_Ip_DmaRxCompleteCallback
Parsed function:Lpuart_0_Uart_Ip_DmaTxCompleteCallback
Parsed function:Lpuart_0_Uart_Ip_DmaRxCompleteCallback
Parsed function:LPUART_UART_IP_2_IRQHandler
Parsed function:LPUART_UART_IP_1_IRQHandler
Parsed function:LPUART_UART_IP_0_IRQHandler
Dump after hash based groups
Congruence classes: 6 (unique hash values: 6), with total: 9 items
Class size histogram [num of members]: number of classe number of classess
[1]: 3 classes
[2]: 3 classes


Dump after WPA based types groups
Congruence classes: 9 (unique hash values: 6), with total: 9 items
Class size histogram [num of members]: number of classe number of classess
[1]: 9 classes


Worklist has been filled with: 0
Address reference subdivision created: 0 new classes.
Dump after callgraph-based congruence reduction
Congruence classes: 9 (unique hash values: 6), with total: 9 items
Class size histogram [num of members]: number of classe number of classess
[1]: 9 classes


Init called for 0 items (0.00%).
Dump after full equality comparison of groups
Congruence classes: 9 (unique hash values: 6), with total: 9 items
Class size histogram [num of members]: number of classe number of classess
[1]: 9 classes


Worklist has been filled with: 0
Address reference subdivision created: 0 new classes.
Congruence classes: 9 (unique hash values: 6), with total: 9 items
Class size histogram [num of members]: number of classe number of classess
[1]: 9 classes



Item count: 9
Congruent classes before: 9, after: 9
Average class size before: 1.00, after: 1.00
Average non-singular class size: 0.00, count: 0
Equal symbols: 0
Fraction of visited symbols: 0.00%

Lpuart_2_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_CompleteSendUsingDma (2);
  return;

}


Lpuart_2_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_CompleteReceiveUsingDma (2);
  return;

}


Lpuart_1_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_CompleteSendUsingDma (1);
  return;

}


Lpuart_1_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_CompleteReceiveUsingDma (1);
  return;

}


Lpuart_0_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_CompleteSendUsingDma (0);
  return;

}


Lpuart_0_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_CompleteReceiveUsingDma (0);
  return;

}


LPUART_UART_IP_2_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_IrqHandler (2);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


LPUART_UART_IP_1_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_IrqHandler (1);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


LPUART_UART_IP_0_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Uart_Ip_IrqHandler (0);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


