
Analyzing function: Flexio_3_Uart_Ip_DmaTxCompleteCallback/7
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Flexio_3_Uart_Ip_DmaTxCompleteCallback

IPA function summary for Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 inlinable
  global time:     13.000000
  self size:       5
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant


Analyzing function: Flexio_3_Uart_Ip_DmaRxCompleteCallback/6
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Flexio_3_Uart_Ip_DmaRxCompleteCallback

IPA function summary for Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 inlinable
  global time:     13.000000
  self size:       5
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant


Analyzing function: Flexio_2_Uart_Ip_DmaTxCompleteCallback/5
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Flexio_2_Uart_Ip_DmaTxCompleteCallback

IPA function summary for Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 inlinable
  global time:     13.000000
  self size:       5
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant


Analyzing function: Flexio_2_Uart_Ip_DmaRxCompleteCallback/4
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Flexio_2_Uart_Ip_DmaRxCompleteCallback

IPA function summary for Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 inlinable
  global time:     13.000000
  self size:       5
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant


Analyzing function: Flexio_1_Uart_Ip_DmaTxCompleteCallback/3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Flexio_1_Uart_Ip_DmaTxCompleteCallback

IPA function summary for Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 inlinable
  global time:     13.000000
  self size:       5
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant


Analyzing function: Flexio_1_Uart_Ip_DmaRxCompleteCallback/2
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Flexio_1_Uart_Ip_DmaRxCompleteCallback

IPA function summary for Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 inlinable
  global time:     13.000000
  self size:       5
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant


Analyzing function: Flexio_0_Uart_Ip_DmaTxCompleteCallback/1
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Flexio_0_Uart_Ip_DmaTxCompleteCallback

IPA function summary for Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 inlinable
  global time:     13.000000
  self size:       5
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteSendUsingDma/9 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant


Analyzing function: Flexio_0_Uart_Ip_DmaRxCompleteCallback/0
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Flexio_0_Uart_Ip_DmaRxCompleteCallback

IPA function summary for Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 inlinable
  global time:     13.000000
  self size:       5
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Flexio_Uart_Ip_CompleteReceiveUsingDma/8 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11
       op0 is compile time invariant

Symbol table:

Flexio_Uart_Ip_CompleteSendUsingDma/9 (Flexio_Uart_Ip_CompleteSendUsingDma) @05df57e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 (1073741824 (estimated locally),1.00 per call) Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 (1073741824 (estimated locally),1.00 per call) Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 (1073741824 (estimated locally),1.00 per call) Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (Flexio_Uart_Ip_CompleteReceiveUsingDma) @05df5620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 (1073741824 (estimated locally),1.00 per call) Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 (1073741824 (estimated locally),1.00 per call) Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 (1073741824 (estimated locally),1.00 per call) Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Flexio_3_Uart_Ip_DmaTxCompleteCallback/7 (Flexio_3_Uart_Ip_DmaTxCompleteCallback) @05df51c0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 (1073741824 (estimated locally),1.00 per call) 
Flexio_3_Uart_Ip_DmaRxCompleteCallback/6 (Flexio_3_Uart_Ip_DmaRxCompleteCallback) @05df1e00
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (1073741824 (estimated locally),1.00 per call) 
Flexio_2_Uart_Ip_DmaTxCompleteCallback/5 (Flexio_2_Uart_Ip_DmaTxCompleteCallback) @05df18c0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 (1073741824 (estimated locally),1.00 per call) 
Flexio_2_Uart_Ip_DmaRxCompleteCallback/4 (Flexio_2_Uart_Ip_DmaRxCompleteCallback) @05df1380
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (1073741824 (estimated locally),1.00 per call) 
Flexio_1_Uart_Ip_DmaTxCompleteCallback/3 (Flexio_1_Uart_Ip_DmaTxCompleteCallback) @05df1d20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 (1073741824 (estimated locally),1.00 per call) 
Flexio_1_Uart_Ip_DmaRxCompleteCallback/2 (Flexio_1_Uart_Ip_DmaRxCompleteCallback) @05df1a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (1073741824 (estimated locally),1.00 per call) 
Flexio_0_Uart_Ip_DmaTxCompleteCallback/1 (Flexio_0_Uart_Ip_DmaTxCompleteCallback) @05df17e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteSendUsingDma/9 (1073741824 (estimated locally),1.00 per call) 
Flexio_0_Uart_Ip_DmaRxCompleteCallback/0 (Flexio_0_Uart_Ip_DmaRxCompleteCallback) @05df1540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Flexio_Uart_Ip_CompleteReceiveUsingDma/8 (1073741824 (estimated locally),1.00 per call) 
Flexio_3_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (3);
  return;

}


Flexio_3_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (3);
  return;

}


Flexio_2_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (2);
  return;

}


Flexio_2_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (2);
  return;

}


Flexio_1_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (1);
  return;

}


Flexio_1_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (1);
  return;

}


Flexio_0_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (0);
  return;

}


Flexio_0_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (0);
  return;

}


