;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1

Symbols to be put in SSA form
{ D.6114 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 7
Number of blocks to update: 6 ( 86%)


;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1

Symbols to be put in SSA form
{ D.6121 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 11
Number of blocks to update: 10 ( 91%)


IntIrqDispatcher.constprop (const uint32 LocHwCh)
{
  uint32 chIntStatus;
  const uint32 LocHwVers;
  const uint32 LocHwInst;
  long unsigned int _1;
  long unsigned int _3;
  short unsigned int _5;
  short unsigned int _6;
  unsigned char _7;

  <bb 6> [local count: 1073741824]:
  # DEBUG LocHwInst => 0
  # DEBUG LocHwVers => 2

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(struct Dma_Ip_Hwv2InstRegType *)1073774592B].reg_INT;
  _3 = 1 << LocHwCh_2(D);
  chIntStatus_4 = _1 & _3;
  # DEBUG chIntStatus => chIntStatus_4
  # DEBUG BEGIN_STMT
  _5 = MEM[(struct Dma_Ip_Hwv2TcdArrayType *)1073778688B].TCD_RSV[LocHwCh_2(D)].tChTcdReg.tTcdReg.reg_CSR;
  _6 = _5 & 6;
  # DEBUG chIntEnable => (uint32) _6
  # DEBUG BEGIN_STMT
  if (chIntStatus_4 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _7 = (unsigned char) LocHwCh_2(D);
  MEM[(struct Dma_Ip_Hwv2InstRegType *)1073774592B].reg_CINT ={v} _7;
  # DEBUG BEGIN_STMT
  if (_6 != 0)
    goto <bb 4>; [33.00%]
  else
    goto <bb 5>; [67.00%]

  <bb 4> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  Dma_Ip_IntIrqHandler (2, 0, LocHwCh_2(D));

  <bb 5> [local count: 1073741824]:
  return;

}


Dma_Ch0_Ch15_ErrorIrqDispatcher.constprop ()
{
  uint32 LocHwCh;
  uint32 TmpHwCh;
  volatile uint32 chErrStatus;
  volatile uint32 chErrEnable;
  const uint32 LocHwVers;
  const uint32 LocHwInst;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int chErrStatus.0_7;
  long unsigned int chErrEnable.1_8;
  unsigned char _9;

  <bb 10> [local count: 63136020]:
  # DEBUG LocHwInst => 0
  # DEBUG LocHwVers => 2

  <bb 2> [local count: 63136020]:
  # DEBUG BEGIN_STMT
  # DEBUG LocHwCh => 0
  # DEBUG BEGIN_STMT
  # DEBUG TmpHwCh => 0
  # DEBUG BEGIN_STMT
  chErrStatus ={v} 0;
  # DEBUG BEGIN_STMT
  chErrEnable ={v} 0;
  # DEBUG BEGIN_STMT
  # DEBUG LocHwCh => 0
  goto <bb 8>; [100.00%]

  <bb 3> [local count: 1010605805]:
  # DEBUG BEGIN_STMT
  TmpHwCh_2 = 1 << LocHwCh_1;
  # DEBUG TmpHwCh => TmpHwCh_2
  # DEBUG BEGIN_STMT
  _3 ={v} MEM[(struct Dma_Ip_Hwv2InstRegType *)1073774592B].reg_ERR;
  _4 = TmpHwCh_2 & _3;
  chErrStatus ={v} _4;
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(struct Dma_Ip_Hwv2InstRegType *)1073774592B].reg_EEI;
  _6 = TmpHwCh_2 & _5;
  chErrEnable ={v} _6;
  # DEBUG BEGIN_STMT
  chErrStatus.0_7 ={v} chErrStatus;
  if (chErrStatus.0_7 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 4> [local count: 505302902]:
  # DEBUG BEGIN_STMT
  chErrEnable.1_8 ={v} chErrEnable;
  if (chErrEnable.1_8 != 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 166749958]:
  # DEBUG BEGIN_STMT
  Dma_Ip_ErrorIrqHandler (2, 0, LocHwCh_1);

  <bb 6> [local count: 505302902]:
  # DEBUG BEGIN_STMT
  _9 = (unsigned char) LocHwCh_1;
  MEM[(struct Dma_Ip_Hwv2InstRegType *)1073774592B].reg_CERR ={v} _9;

  <bb 7> [local count: 1010605805]:
  # DEBUG BEGIN_STMT
  LocHwCh_10 = LocHwCh_1 + 1;
  # DEBUG LocHwCh => LocHwCh_10

  <bb 8> [local count: 1073741824]:
  # LocHwCh_1 = PHI <0(2), LocHwCh_10(7)>
  # DEBUG LocHwCh => LocHwCh_1
  # DEBUG BEGIN_STMT
  if (LocHwCh_1 != 16)
    goto <bb 3>; [94.12%]
  else
    goto <bb 9>; [5.88%]

  <bb 9> [local count: 63136019]:
  return;

}


Dma0_Error_IrqHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Dma_Ch0_Ch15_ErrorIrqDispatcher (2, 0);
  return;

}


Dma0_Ch15_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 15);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch14_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 14);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch13_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 13);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch12_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 12);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch11_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 11);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch10_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 10);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch9_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 9);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch8_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 8);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch7_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 7);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch6_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 6);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch5_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 5);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch4_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 4);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch3_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 3);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch2_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 2);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch1_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 1);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


Dma0_Ch0_IRQHandler ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  IntIrqDispatcher (2, 0, 0);
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" DSB");
  return;

}


