Parsed function:Flexio_3_Uart_Ip_DmaTxCompleteCallback
Parsed function:Flexio_3_Uart_Ip_DmaRxCompleteCallback
Parsed function:Flexio_2_Uart_Ip_DmaTxCompleteCallback
Parsed function:Flexio_2_Uart_Ip_DmaRxCompleteCallback
Parsed function:Flexio_1_Uart_Ip_DmaTxCompleteCallback
Parsed function:Flexio_1_Uart_Ip_DmaRxCompleteCallback
Parsed function:Flexio_0_Uart_Ip_DmaTxCompleteCallback
Parsed function:Flexio_0_Uart_Ip_DmaRxCompleteCallback
Dump after hash based groups
Congruence classes: 4 (unique hash values: 4), with total: 8 items
Class size histogram [num of members]: number of classe number of classess
[2]: 4 classes


Dump after WPA based types groups
Congruence classes: 8 (unique hash values: 4), with total: 8 items
Class size histogram [num of members]: number of classe number of classess
[1]: 8 classes


Worklist has been filled with: 0
Address reference subdivision created: 0 new classes.
Dump after callgraph-based congruence reduction
Congruence classes: 8 (unique hash values: 4), with total: 8 items
Class size histogram [num of members]: number of classe number of classess
[1]: 8 classes


Init called for 0 items (0.00%).
Dump after full equality comparison of groups
Congruence classes: 8 (unique hash values: 4), with total: 8 items
Class size histogram [num of members]: number of classe number of classess
[1]: 8 classes


Worklist has been filled with: 0
Address reference subdivision created: 0 new classes.
Congruence classes: 8 (unique hash values: 4), with total: 8 items
Class size histogram [num of members]: number of classe number of classess
[1]: 8 classes



Item count: 8
Congruent classes before: 8, after: 8
Average class size before: 1.00, after: 1.00
Average non-singular class size: 0.00, count: 0
Equal symbols: 0
Fraction of visited symbols: 0.00%

Flexio_3_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (3);
  return;

}


Flexio_3_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (3);
  return;

}


Flexio_2_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (2);
  return;

}


Flexio_2_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (2);
  return;

}


Flexio_1_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (1);
  return;

}


Flexio_1_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (1);
  return;

}


Flexio_0_Uart_Ip_DmaTxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteSendUsingDma (0);
  return;

}


Flexio_0_Uart_Ip_DmaRxCompleteCallback ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Flexio_Uart_Ip_CompleteReceiveUsingDma (0);
  return;

}


