<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00046.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Mcl</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Mcl</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T40D2M10I0R0/Mcl</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-PRE-COMPILE</IMPLEMENTATION-CONFIG-VARIANT>
          <POST-BUILD-VARIANT-USED>true</POST-BUILD-VARIANT-USED>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>255</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>MclConfig</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FlexioCommon_0</SHORT-NAME>
                  <INDEX>0</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioDebugEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclInstances</DEFINITION-REF>
                      <VALUE>FLEXIO_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>FLEXIO_RX</SHORT-NAME>
                      <INDEX>0</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels/FlexioMclAddPinEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels/FlexioMclAddPinId</DEFINITION-REF>
                          <VALUE>PIN_1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels/FlexioMclChannelId</DEFINITION-REF>
                          <VALUE>CHANNEL_0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels/FlexioMclPinId</DEFINITION-REF>
                          <VALUE>PIN_6</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>FLEXIO_TX</SHORT-NAME>
                      <INDEX>1</INDEX>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels/FlexioMclAddPinEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels/FlexioMclAddPinId</DEFINITION-REF>
                          <VALUE>PIN_2</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels/FlexioMclChannelId</DEFINITION-REF>
                          <VALUE>CHANNEL_1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/FlexioCommon/FlexioMclLogicChannels/FlexioMclPinId</DEFINITION-REF>
                          <VALUE>PIN_7</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>UART0_RX</SHORT-NAME>
                  <INDEX>0</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableGlobalConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableScatterGather</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableTransferConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ErrorInterruptCallback</DEFINITION-REF>
                      <VALUE>NULL_PTR</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwChId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_CH_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwInstId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_INST_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_InterruptCallback</DEFINITION-REF>
                      <VALUE>Lpuart_0_Uart_Ip_DmaRxCompleteCallback</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_LogicName</DEFINITION-REF>
                      <VALUE>DMA_LOGIC_CH_UART0_RX</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>dmaLogicChannel_ConfigType</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_GlobalConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalInterruptType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType/dmaGlobalInterrupt_enDmaErrorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalPriorityType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_LevelPriority</DEFINITION-REF>
                                  <VALUE>DMA_IP_LEVEL_PRIO0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_disPreempt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_enPreemption</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalRequestType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_Dmamux0HwRequest</DEFINITION-REF>
                                  <VALUE>DMA_IP_REQ_MUX0_LPUART0_RX</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmaRequest</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxSource</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxTrigger</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_ScatterGatherConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_ScatterGatherConfigType</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_TransferConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferControlType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_DestinationStoreAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_ScatterGatherAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_bandwidthControl</DEFINITION-REF>
                                  <VALUE>DMA_IP_BWC_ENGINE_NO_STALL</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_disDmaAutoHwReq</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaHalfMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enStart</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferDestinationType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMajorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_MajorLoopCountType</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_enMajorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMinorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_MinorLoopSizeType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_OffsetValueType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enDestinationOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enMinorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enSourceOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferSourceType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>UART1_RX</SHORT-NAME>
                  <INDEX>1</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableGlobalConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableScatterGather</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableTransferConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ErrorInterruptCallback</DEFINITION-REF>
                      <VALUE>NULL_PTR</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwChId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_CH_1</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwInstId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_INST_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_InterruptCallback</DEFINITION-REF>
                      <VALUE>Lpuart_1_Uart_Ip_DmaRxCompleteCallback</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_LogicName</DEFINITION-REF>
                      <VALUE>DMA_LOGIC_CH_UART1_RX</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>dmaLogicChannel_ConfigType</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_GlobalConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalInterruptType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType/dmaGlobalInterrupt_enDmaErrorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalPriorityType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_LevelPriority</DEFINITION-REF>
                                  <VALUE>DMA_IP_LEVEL_PRIO1</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_disPreempt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_enPreemption</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalRequestType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_Dmamux0HwRequest</DEFINITION-REF>
                                  <VALUE>DMA_IP_REQ_MUX0_LPUART1_RX</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmaRequest</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxSource</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxTrigger</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_ScatterGatherConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_ScatterGatherConfigType</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_TransferConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferControlType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_DestinationStoreAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_ScatterGatherAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_bandwidthControl</DEFINITION-REF>
                                  <VALUE>DMA_IP_BWC_ENGINE_NO_STALL</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_disDmaAutoHwReq</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaHalfMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enStart</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferDestinationType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMajorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_MajorLoopCountType</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_enMajorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMinorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_MinorLoopSizeType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_OffsetValueType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enDestinationOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enMinorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enSourceOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferSourceType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>UART2_RX</SHORT-NAME>
                  <INDEX>2</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableGlobalConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableScatterGather</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableTransferConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ErrorInterruptCallback</DEFINITION-REF>
                      <VALUE>NULL_PTR</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwChId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_CH_2</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwInstId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_INST_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_InterruptCallback</DEFINITION-REF>
                      <VALUE>Lpuart_2_Uart_Ip_DmaRxCompleteCallback</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_LogicName</DEFINITION-REF>
                      <VALUE>DMA_LOGIC_CH_UART2_RX</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>dmaLogicChannel_ConfigType</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_GlobalConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalInterruptType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType/dmaGlobalInterrupt_enDmaErrorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalPriorityType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_LevelPriority</DEFINITION-REF>
                                  <VALUE>DMA_IP_LEVEL_PRIO2</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_disPreempt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_enPreemption</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalRequestType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_Dmamux0HwRequest</DEFINITION-REF>
                                  <VALUE>DMA_IP_REQ_MUX0_LPUART2_RX</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmaRequest</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxSource</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxTrigger</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_ScatterGatherConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_ScatterGatherConfigType</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_TransferConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferControlType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_DestinationStoreAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_ScatterGatherAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_bandwidthControl</DEFINITION-REF>
                                  <VALUE>DMA_IP_BWC_ENGINE_NO_STALL</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_disDmaAutoHwReq</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaHalfMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enStart</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferDestinationType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMajorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_MajorLoopCountType</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_enMajorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMinorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_MinorLoopSizeType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_OffsetValueType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enDestinationOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enMinorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enSourceOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferSourceType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>UART0_TX</SHORT-NAME>
                  <INDEX>3</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableGlobalConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableScatterGather</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableTransferConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ErrorInterruptCallback</DEFINITION-REF>
                      <VALUE>NULL_PTR</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwChId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_CH_3</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwInstId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_INST_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_InterruptCallback</DEFINITION-REF>
                      <VALUE>Lpuart_0_Uart_Ip_DmaTxCompleteCallback</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_LogicName</DEFINITION-REF>
                      <VALUE>DMA_LOGIC_CH_UART0_TX</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>dmaLogicChannel_ConfigType</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_GlobalConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalInterruptType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType/dmaGlobalInterrupt_enDmaErrorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalPriorityType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_LevelPriority</DEFINITION-REF>
                                  <VALUE>DMA_IP_LEVEL_PRIO3</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_disPreempt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_enPreemption</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalRequestType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_Dmamux0HwRequest</DEFINITION-REF>
                                  <VALUE>DMA_IP_REQ_MUX0_LPUART0_TX</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmaRequest</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxSource</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxTrigger</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_ScatterGatherConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_ScatterGatherConfigType</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_TransferConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferControlType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_DestinationStoreAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_ScatterGatherAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_bandwidthControl</DEFINITION-REF>
                                  <VALUE>DMA_IP_BWC_ENGINE_NO_STALL</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_disDmaAutoHwReq</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaHalfMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enStart</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferDestinationType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMajorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_MajorLoopCountType</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_enMajorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMinorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_MinorLoopSizeType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_OffsetValueType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enDestinationOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enMinorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enSourceOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferSourceType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>UART1_TX</SHORT-NAME>
                  <INDEX>4</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableGlobalConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableScatterGather</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableTransferConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ErrorInterruptCallback</DEFINITION-REF>
                      <VALUE>NULL_PTR</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwChId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_CH_4</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwInstId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_INST_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_InterruptCallback</DEFINITION-REF>
                      <VALUE>Lpuart_1_Uart_Ip_DmaTxCompleteCallback</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_LogicName</DEFINITION-REF>
                      <VALUE>DMA_LOGIC_CH_UART1_TX</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>dmaLogicChannel_ConfigType</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_GlobalConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalInterruptType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType/dmaGlobalInterrupt_enDmaErrorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalPriorityType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_LevelPriority</DEFINITION-REF>
                                  <VALUE>DMA_IP_LEVEL_PRIO4</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_disPreempt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_enPreemption</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalRequestType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_Dmamux0HwRequest</DEFINITION-REF>
                                  <VALUE>DMA_IP_REQ_MUX0_LPUART1_TX</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmaRequest</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxSource</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxTrigger</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_ScatterGatherConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_ScatterGatherConfigType</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_TransferConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferControlType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_DestinationStoreAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_ScatterGatherAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_bandwidthControl</DEFINITION-REF>
                                  <VALUE>DMA_IP_BWC_ENGINE_NO_STALL</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_disDmaAutoHwReq</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaHalfMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enStart</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferDestinationType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMajorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_MajorLoopCountType</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_enMajorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMinorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_MinorLoopSizeType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_OffsetValueType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enDestinationOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enMinorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enSourceOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferSourceType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>UART2_TX</SHORT-NAME>
                  <INDEX>5</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableGlobalConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableScatterGather</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_EnableTransferConfig</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ErrorInterruptCallback</DEFINITION-REF>
                      <VALUE>NULL_PTR</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwChId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_CH_5</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_HwInstId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_INST_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_InterruptCallback</DEFINITION-REF>
                      <VALUE>Lpuart_2_Uart_Ip_DmaTxCompleteCallback</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_LogicName</DEFINITION-REF>
                      <VALUE>DMA_LOGIC_CH_UART2_TX</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>dmaLogicChannel_ConfigType</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_GlobalConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalInterruptType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalInterruptType/dmaGlobalInterrupt_enDmaErrorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalPriorityType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_LevelPriority</DEFINITION-REF>
                                  <VALUE>DMA_IP_LEVEL_PRIO5</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_disPreempt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalPriorityType/dmaGlobalPriority_enPreemption</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_GlobalRequestType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_Dmamux0HwRequest</DEFINITION-REF>
                                  <VALUE>DMA_IP_REQ_MUX0_LPUART2_TX</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmaRequest</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxSource</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_GlobalConfigType/dmaLogicChannelConfig_GlobalRequestType/dmaGlobalRequest_enDmamuxTrigger</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_ScatterGatherConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_ScatterGatherConfigType</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>dmaLogicChannel_TransferConfigType</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferControlType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_DestinationStoreAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_ScatterGatherAddressType</DEFINITION-REF>
                                  <VALUE>0U</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_bandwidthControl</DEFINITION-REF>
                                  <VALUE>DMA_IP_BWC_ENGINE_NO_STALL</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_disDmaAutoHwReq</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaHalfMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enDmaMajorInterrupt</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferControlType/dmaLogicChannelConfig_enStart</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferDestinationType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaLogicChannelConfig_DestinationSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferDestinationType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMajorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_MajorLoopCountType</DEFINITION-REF>
                                  <VALUE>1</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMajorLoopType/dmaLogicChannelConfig_enMajorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferMinorLoopType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_MinorLoopSizeType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_OffsetValueType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enDestinationOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enMinorLoopLinkCh</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferMinorLoopType/dmaLogicChannelConfig_enSourceOffset</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>dmaLogicChannelConfig_TransferSourceType</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType</DEFINITION-REF>
                              <PARAMETER-VALUES>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceAddressType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceLastAddressAdjustmentType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceModuloType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-NUMERICAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaLogicChannelConfig_SourceSignedOffsetType</DEFINITION-REF>
                                  <VALUE>0</VALUE>
                                </ECUC-NUMERICAL-PARAM-VALUE>
                                <ECUC-TEXTUAL-PARAM-VALUE>
                                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicChannel_Type/dmaLogicChannel_ConfigType/dmaLogicChannel_TransferConfigType/dmaLogicChannelConfig_TransferSourceType/dmaTransferConfig_TransferSizeType</DEFINITION-REF>
                                  <VALUE>DMA_IP_TRANSFER_SIZE_1_BYTE</VALUE>
                                </ECUC-TEXTUAL-PARAM-VALUE>
                              </PARAMETER-VALUES>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>dmaLogicInstance_ConfigType_0</SHORT-NAME>
                  <INDEX>0</INDEX>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicInstance_ConfigType</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicInstance_ConfigType/dmaLogicInstance_IdName</DEFINITION-REF>
                      <VALUE>DMA_LOGIC_INST_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicInstance_ConfigType/dmaLogicInstance_enChLinking</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicInstance_ConfigType/dmaLogicInstance_enDebug</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicInstance_ConfigType/dmaLogicInstance_enHaltAfterError</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicInstance_ConfigType/dmaLogicInstance_enRoundRobin</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclConfig/dmaLogicInstance_ConfigType/dmaLogicInstance_hwId</DEFINITION-REF>
                      <VALUE>DMA_IP_HW_INST_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>MclGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclEnableDemReportErrorStatus</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclEnableDevErrorDetect</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclEnableUserModeSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclEnableVirtualAddressMappingSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/Mcl_VersionInfoApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MclCache</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclCache</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclCache/MclCacheTimeoutMethod</DEFINITION-REF>
                      <VALUE>OSIF_COUNTER_DUMMY</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclCache/MclCacheTimeoutValue</DEFINITION-REF>
                      <VALUE>100000</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclCache/MclEnableCache</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MclDma</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclDma</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclDma/MclEnableDma</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MclFlexioCommon</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclFlexioCommon</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclFlexioCommon/MclEnableFlexioCommon</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MclFtmCommon</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclFtmCommon</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclFtmCommon/Mcl_FtmCommonTimebase</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MclTrgMux</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclTrgMux</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcl/MclGeneral/MclTrgMux/MclEnableTrgMux</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
