<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00046.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Port</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Port</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T40D2M10I0R0/Port</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-PRE-COMPILE</IMPLEMENTATION-CONFIG-VARIANT>
          <POST-BUILD-VARIANT-USED>true</POST-BUILD-VARIANT-USED>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>124</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>PortConfigSet</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>NotUsedPortPin</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/NotUsedPortPin</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/NotUsedPortPin/PortPinDSE</DEFINITION-REF>
                      <VALUE>Low_Drive_Strength</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/NotUsedPortPin/PortPinDirection</DEFINITION-REF>
                      <VALUE>PORT_PIN_IN</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/NotUsedPortPin/PortPinLevelValue</DEFINITION-REF>
                      <VALUE>PORT_PIN_LEVEL_LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/NotUsedPortPin/PortPinMode</DEFINITION-REF>
                      <VALUE>GPIO</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/NotUsedPortPin/PortPinPE</DEFINITION-REF>
                      <VALUE>PullDisabled</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/NotUsedPortPin/PortPinPS</DEFINITION-REF>
                      <VALUE>PullDown</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>PortContainer_CAN</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortNumberOfPortPins</DEFINITION-REF>
                      <VALUE>4</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTA12_CAN1_RX_MCU_CAN1_RX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_IN</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>17</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>CAN1_RX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>12</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTA13_CAN1_TX_MCU_CAN1_TX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>16</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>CAN1_TX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>13</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTE4_CAN0_RX_MCU_CAN0_RX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_IN</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>8</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>CAN0_RX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullUp</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>132</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTE5_CAN0_TX_MCU_CAN0_TX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>CAN0_TX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullUp</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>133</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>PortContainer_GPIO</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortNumberOfPortPins</DEFINITION-REF>
                      <VALUE>7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTC6_GPIO_IN_MCU_HVIL</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_IN</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>15</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>GPIO</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullEnabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullUp</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>70</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTC7_GPIO_IN_MCU_DISPLACE</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_IN</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>14</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>GPIO</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullEnabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullUp</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>71</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTD15_GPIO_OUT_MCU_WIFI_RESET</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>10</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>GPIO</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>111</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTD16_GPIO_OUT_MCU_WIFI_POW_EN</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>9</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_LOW</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>GPIO</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>112</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTE7_GPIO_OUT_MCU_BT_MOD</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>13</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_LOW</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>GPIO</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>135</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTE8_GPIO_OUT_MCU_BT_RESET</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>12</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>GPIO</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>136</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTE9_GPIO_OUT_MCU_BT_POW_EN</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>High_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>11</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_LOW</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>GPIO</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>137</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>PortContainer_LPUART</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortNumberOfPortPins</DEFINITION-REF>
                      <VALUE>6</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTC2_LPUART0_RX_MCU_RXD0_RX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_IN</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>LPUART0_RX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>66</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTC3_LPUART0_TX_MCU_TXD0_TX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>LPUART0_TX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>67</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTC8_LPUART1_RX_MCU_WIFI_RX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_IN</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>4</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>LPUART1_RX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>72</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTC9_LPUART1_TX_MCU_WIFI_TX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>3</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>LPUART1_TX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>73</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTD6_LPUART2_RX_MCU_BT_RX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_IN</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>6</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>LPUART2_RX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>102</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>PTD7_LPUART2_TX_MCU_BT_TX</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDSE</DEFINITION-REF>
                          <VALUE>Low_Drive_Strength</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirection</DEFINITION-REF>
                          <VALUE>PORT_PIN_OUT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinDirectionChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinId</DEFINITION-REF>
                          <VALUE>5</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinInitialMode</DEFINITION-REF>
                          <VALUE>PORT_GPIO_MODE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLK</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinLevelValue</DEFINITION-REF>
                          <VALUE>PORT_PIN_LEVEL_HIGH</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinMode</DEFINITION-REF>
                          <VALUE>LPUART2_TX</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinModeChangeable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPE</DEFINITION-REF>
                          <VALUE>PullDisabled</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPFE</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPS</DEFINITION-REF>
                          <VALUE>PullDown</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/PortContainer/PortPin/PortPinPcr</DEFINITION-REF>
                          <VALUE>103</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>EXTAL</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin/PortPinPcr</DEFINITION-REF>
                      <VALUE>39</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>JTAG_TCK</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin/PortPinPcr</DEFINITION-REF>
                      <VALUE>68</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>JTAG_TDI</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin/PortPinPcr</DEFINITION-REF>
                      <VALUE>69</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>JTAG_TDO</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin/PortPinPcr</DEFINITION-REF>
                      <VALUE>10</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>JTAG_TMS</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin/PortPinPcr</DEFINITION-REF>
                      <VALUE>4</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>Reset_b</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin/PortPinPcr</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>XTAL</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortConfigSet/UnTouchedPortPin/PortPinPcr</DEFINITION-REF>
                      <VALUE>38</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>PortGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Port/PortGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortCiPortIPDevErrorDetect</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortDevErrorDetect</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortEnableUserModeSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortMulticoreSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortResetPinModeApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortSet2PinsDirectionApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortSetAsUnusedPinApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortSetPinDirectionApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortSetPinModeApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortSetPinModeDoesNotTouchGpioLevel</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Port/PortGeneral/PortVersionInfoApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
