<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00046.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Dem</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Dem</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T40D2M10I0R0/Dem</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-PRE-COMPILE</IMPLEMENTATION-CONFIG-VARIANT>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>54</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>DemConfigSet</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>DemComponent_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemComponent</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemComponent/DemComponentIgnoresPriority</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_ERASE_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>4</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_READ_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_UNEXPECTED_FLASH_ID</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_WRITE_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>3</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>GPT_E_FORBIDDEN_INVOCATION</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>24</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>GPT_E_PERIODIC_CHECK</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>25</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCEM_E_ERROR</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>6</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCEM_E_ERROR_BACK</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCL_DMA_E_BUS</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>20</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCL_DMA_E_DESCRIPTOR</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>20</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCL_DMA_E_ECC</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>20</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCL_DMA_E_PRIORITY</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>20</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_CER_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>19</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_CLOCK_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_DEFAULTCASE_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>2</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_DESTRESET_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>12</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_FORBIDDEN_INVOCATION</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>3</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_FUNCRESET_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>4</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_INVALIDMODE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>15</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_INVALIDMODE_CONFIG</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>16</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_INVALID_PARAMETER</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_LOCK_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>11</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_MEMORY_CORRUPTION</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>6</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_MODE_TRANSTION_COMPLETE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>14</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_PLLLOCK_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_QUARTZ_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>8</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_SAFEMODE_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>13</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_SPURIOUSINT_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>9</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_SSCM_CER_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>20</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_SWITCHMODE_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>10</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_TEMPERATURE_ERROR</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>18</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_TIMEOUT_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>11</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_TIMEOUT_TRANSITION</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>13</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_VOLTAGE_ERROR</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>17</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_CORRUPT_CONFIG</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>19</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_DISABLE_REJECTED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>17</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_FORBIDDEN_INVOCATION</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>22</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_FORBIDEN_INVOCATION</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>22</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_INVALID_CALL</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>23</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_INVALID_PARAMETER</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>21</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_MEMORY_CORRUPTION</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>19</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_MISS_TRIGGER</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>18</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_MODE_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>16</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                          <SUB-CONTAINERS>
                            <ECUC-CONTAINER-VALUE>
                              <SHORT-NAME>DemCallbackGetFDC</SHORT-NAME>
                              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal/DemCallbackGetFDC</DEFINITION-REF>
                            </ECUC-CONTAINER-VALUE>
                          </SUB-CONTAINERS>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_UNLOCKED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>20</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemGeneral/DemOperationCycle_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceMonitorInternal</DEFINITION-REF>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>DemGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemAgingCycleCounterProcessing</DEFINITION-REF>
                  <VALUE>DEM_PROCESS_AGINGCTR_EXTERN</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemAgingRequieresTestedCycle</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemAvailabilitySupport</DEFINITION-REF>
                  <VALUE>DEM_EVENT_AVAILABILITY</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemBswErrorBufferSize</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemClearDTCBehavior</DEFINITION-REF>
                  <VALUE>DEM_CLRRESP_NONVOLATILE_FINISH</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemClearDTCLimitation</DEFINITION-REF>
                  <VALUE>DEM_ALL_SUPPORTED_DTCS</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemDataElementDefaultEndianness</DEFINITION-REF>
                  <VALUE>BIG_ENDIAN</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemDebounceCounterBasedSupport</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemDebounceTimeBasedSupport</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemDevErrorDetect</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemDtcStatusAvailabilityMask</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemEventCombinationSupport</DEFINITION-REF>
                  <VALUE>DEM_EVCOMB_DISABLED</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemEventDisplacementStrategy</DEFINITION-REF>
                  <VALUE>DEM_DISPLACEMENT_FULL</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemEventMemoryEntryStorageTrigger</DEFINITION-REF>
                  <VALUE>DEM_TRIGGER_ON_CONFIRMED</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemGeneralInterfaceSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemMaxNumberEventEntryPermanent</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemMaxNumberPrestoredFF</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemOBDSupport</DEFINITION-REF>
                  <VALUE>DEM_OBD_DEP_SEC_ECU</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemOccurrenceCounterProcessing</DEFINITION-REF>
                  <VALUE>DEM_PROCESS_OCCCTR_CDTC</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemOperationCycleStatusStorage</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemPTOSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemResetConfirmedBitOnOverflow</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemStatusBitHandlingTestFailedSinceLastClear</DEFINITION-REF>
                  <VALUE>DEM_STATUS_BIT_AGING_AND_DISPLACEMENT</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemStatusBitStorageTestFailed</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemSuppressionSupport</DEFINITION-REF>
                  <VALUE>DEM_DTC_SUPPRESSION</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemTaskTime</DEFINITION-REF>
                  <VALUE>0.01</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemTriggerDcmReports</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemTriggerDltReports</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemTriggerFiMReports</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemTriggerMonitorInitBeforeClearOk</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemTypeOfDTCSupported</DEFINITION-REF>
                  <VALUE>DEM_DTC_TRANSLATION_ISO11992_4</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemTypeOfFreezeFrameRecordNumeration</DEFINITION-REF>
                  <VALUE>DEM_FF_RECNUM_CALCULATED</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemVersionInfoApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>DemOperationCycle_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemOperationCycle</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemOperationCycle/DemOperationCycleAutomaticEnd</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemOperationCycle/DemOperationCycleAutostart</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemOperationCycle/DemOperationCycleType</DEFINITION-REF>
                      <VALUE>DEM_OPCYC_IGNITION</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>DemPrimaryMemory</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemPrimaryMemory</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Dem/DemGeneral/DemPrimaryMemory/DemMaxNumberEventEntryPrimary</DEFINITION-REF>
                      <VALUE>255</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
