<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00046.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Mcu</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Mcu</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T40D2M10I0R0/Mcu</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-PRE-COMPILE</IMPLEMENTATION-CONFIG-VARIANT>
          <POST-BUILD-VARIANT-USED>true</POST-BUILD-VARIANT-USED>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>101</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/VendorApiInfix</DEFINITION-REF>
                  <VALUE></VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>McuDebugConfiguration</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuDebugConfiguration</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuDebugConfiguration/McuDisableCmuApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuDebugConfiguration/McuDisableDemReportErrorStatus</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuDebugConfiguration/McuEnablePeripheralCMU</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuDebugConfiguration/McuGetClockFrequencyApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuDebugConfiguration/McuGetMidrStructureApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuDebugConfiguration/McuGetPowerModeStatetApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuDebugConfiguration/McuSRAMRetentionConfigApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>McuGeneralConfiguration</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuCalloutBeforePerformReset</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuCmuErrorIsrUsed</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuDevErrorDetect</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuDisablePmcInit</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuDisableRcmInit</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuDisableSmcInit</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuEnableModeChangeNotification</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuEnableUserModeSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuEnterLowPowerMode</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuGetRamStateApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuInitClock</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuNoPll</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuPerformResetApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuPerformResetCallout</DEFINITION-REF>
                  <VALUE>NULL_PTR</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuTimeout</DEFINITION-REF>
                  <VALUE>50000</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuTimeoutMethod</DEFINITION-REF>
                  <VALUE>OSIF_COUNTER_DUMMY</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuGeneralConfiguration/McuVersionInfoApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>McuModuleConfiguration</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSrcFailureNotification</DEFINITION-REF>
                  <VALUE>DISABLED</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuNumberOfMcuModes</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuRTC_CLKINFrequencyHz</DEFINITION-REF>
                  <VALUE>32000.0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuRamSectors</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuTCLK0_REF_CLKFrequencyHz</DEFINITION-REF>
                  <VALUE>0.0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuTCLK1_REF_CLKFrequencyHz</DEFINITION-REF>
                  <VALUE>0.0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuTCLK2_REF_CLKFrequencyHz</DEFINITION-REF>
                  <VALUE>0.0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>McuAllowedModes</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuAllowedModes</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuAllowedModes/McuAllowHighSpeedRunMode</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuAllowedModes/McuAllowVeryLowPowerModes</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>McuClockSettingConfig_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockSettingId</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuScgClkOutSelect</DEFINITION-REF>
                      <VALUE>SPLL_CLK</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSysClockUnderMcuControl</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClkMonitor</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>McuClkMonitor_0</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_0</DEFINITION-REF>
                          <PARAMETER-VALUES>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_0/McuAsyncFHHInterruptEn</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_0/McuAsyncFLLInterruptEn</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_0/McuClkMonitorEn</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_0/McuClockMonitorUnderMcuControl</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_0/McuCmuName</DEFINITION-REF>
                              <VALUE>CMU_FC_0_FIRC_MON1_CLK</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                          </PARAMETER-VALUES>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>McuClkMonitor_1</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_1</DEFINITION-REF>
                          <PARAMETER-VALUES>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_1/McuClkMonitorEn</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_1/McuClockMonitorUnderMcuControl</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_1/McuCmuName</DEFINITION-REF>
                              <VALUE>CMU_FC_1_FIRC_MON2_CLK</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_1/McuSyncFHHInterruptEn</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClkMonitor/McuClkMonitor_1/McuSyncFLLInterruptEn</DEFINITION-REF>
                              <VALUE>0</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                          </PARAMETER-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>RUN_SYS_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_CAN</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>CUSTOM</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_FLEXIO_CLK</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>SIRCDIV2_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_GPT</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>SOSCDIV1_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_LPUART0_CLK</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>LPUART0_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_LPUART1_CLK</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>LPUART1_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_LPUART2_CLK</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>LPUART2_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_WDG</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>LPO_128K_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>128000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuClockReferencePoint_WDG_43</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockFrequencySelect</DEFINITION-REF>
                          <VALUE>LPO_1K_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint/McuClockReferencePointFrequency</DEFINITION-REF>
                          <VALUE>1000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuFIRCClockConfig</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCDiv1</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCDiv1Frequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCDiv2</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCDiv2Frequency</DEFINITION-REF>
                          <VALUE>2.4E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCRangeSelect</DEFINITION-REF>
                          <VALUE>TRIMMED_TO_48MHZ</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCRegulatorEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuFIRCClockConfig/McuFIRCUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuHsrunClockConfig</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuBusClockDivider</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuBusClockFrequency</DEFINITION-REF>
                          <VALUE>2.4E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuCoreClockDivider</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuCoreClockFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuFlashClockFrequency</DEFINITION-REF>
                          <VALUE>1.2E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuPreDivSystemClockFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuScgClkOutFrequency</DEFINITION-REF>
                          <VALUE>9.6E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuSlowClockDivider</DEFINITION-REF>
                          <VALUE>4</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuSystemClockFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuHsrunClockConfig/McuSystemClockSwitch</DEFINITION-REF>
                          <VALUE>SPLL_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FTFC</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_1</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>DMAMUX0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_10</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>PDB1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_11</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>CRC0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_12</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>PDB0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_13</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPIT0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>SIRC</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_14</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FTM0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>SOSC</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_15</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FTM1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_16</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FTM2</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_17</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>ADC0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_18</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>RTC0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_19</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPTMR0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_2</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FLEXCAN0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_20</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>PORTA</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_21</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>PORTB</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_22</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>PORTC</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_23</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>PORTD</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_24</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>PORTE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_25</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FlexIO</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>SIRC</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_26</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>EWM0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_27</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPI2C0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_28</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPUART0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>SOSC</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_29</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPUART1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>SOSC</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_3</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FLEXCAN1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_30</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPUART2</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>SOSC</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_31</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FTM4</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_32</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FTM5</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_33</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>CMP0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_4</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FTM3</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_5</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>ADC1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_6</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>FLEXCAN2</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_7</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPSPI0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_8</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPSPI1</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuPeripheralClockConfig_9</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPerName</DEFINITION-REF>
                          <VALUE>LPSPI2</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockSelect</DEFINITION-REF>
                          <VALUE>CLOCK_IS_OFF</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralClockUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuPeripheralClockConfig/McuPeripheralFractionalDivider</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuRunClockConfig</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuBusClockDivider</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuBusClockFrequency</DEFINITION-REF>
                          <VALUE>2.4E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuCoreClockDivider</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuCoreClockFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuFlashClockFrequency</DEFINITION-REF>
                          <VALUE>1.2E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuPreDivSystemClockFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuScgClkOutFrequency</DEFINITION-REF>
                          <VALUE>9.6E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuSlowClockDivider</DEFINITION-REF>
                          <VALUE>4</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuSystemClockFrequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuRunClockConfig/McuSystemClockSwitch</DEFINITION-REF>
                          <VALUE>SPLL_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuSIMClockConfig</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuDMAClockGatingEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuEIMClockGatingEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuERMClockGatingEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuGPIOClockGatingEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuMPUClockGatingEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuMSCMClockGatingEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSIMUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>McuSimChipConfiguration</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimChipConfiguration</DEFINITION-REF>
                          <PARAMETER-VALUES>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimChipConfiguration/McuCLKOUTDivider</DEFINITION-REF>
                              <VALUE>4</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimChipConfiguration/McuCLKOUTEnable</DEFINITION-REF>
                              <VALUE>1</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimChipConfiguration/McuCLKOUTSelect</DEFINITION-REF>
                              <VALUE>SCG_CLKOUT_CLK</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimChipConfiguration/McuDebugTraceDividerEnable</DEFINITION-REF>
                              <VALUE>1</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimChipConfiguration/McuTRACECLKDivider</DEFINITION-REF>
                              <VALUE>1</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimChipConfiguration/McuTRACECLKFraction</DEFINITION-REF>
                              <VALUE>1</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimChipConfiguration/McuTRACECLKSelect</DEFINITION-REF>
                              <VALUE>CORE_CLK</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                          </PARAMETER-VALUES>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>McuSimFtmConfiguration</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration</DEFINITION-REF>
                          <PARAMETER-VALUES>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration/McuFTM0ExternalClockPinSelect</DEFINITION-REF>
                              <VALUE>TCLK0_PIN</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration/McuFTM1ExternalClockPinSelect</DEFINITION-REF>
                              <VALUE>TCLK0_PIN</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration/McuFTM2ExternalClockPinSelect</DEFINITION-REF>
                              <VALUE>TCLK0_PIN</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration/McuFTM3ExternalClockPinSelect</DEFINITION-REF>
                              <VALUE>TCLK0_PIN</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration/McuFTM4ExternalClockPinSelect</DEFINITION-REF>
                              <VALUE>TCLK0_PIN</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration/McuFTM5ExternalClockPinSelect</DEFINITION-REF>
                              <VALUE>TCLK0_PIN</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration/McuFTM6ExternalClockPinSelect</DEFINITION-REF>
                              <VALUE>TCLK0_PIN</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimFtmConfiguration/McuFTM7ExternalClockPinSelect</DEFINITION-REF>
                              <VALUE>TCLK0_PIN</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                          </PARAMETER-VALUES>
                        </ECUC-CONTAINER-VALUE>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>McuSimLpoConfiguration</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimLpoConfiguration</DEFINITION-REF>
                          <PARAMETER-VALUES>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimLpoConfiguration/McuLPOClkSelect</DEFINITION-REF>
                              <VALUE>LPO_128K_CLK</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimLpoConfiguration/McuLPO_1KClockEnable</DEFINITION-REF>
                              <VALUE>1</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-NUMERICAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimLpoConfiguration/McuLPO_32KClockEnable</DEFINITION-REF>
                              <VALUE>1</VALUE>
                            </ECUC-NUMERICAL-PARAM-VALUE>
                            <ECUC-TEXTUAL-PARAM-VALUE>
                              <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIMClockConfig/McuSimLpoConfiguration/McuRTCClkSelect</DEFINITION-REF>
                              <VALUE>SOSCDIV1_CLK</VALUE>
                            </ECUC-TEXTUAL-PARAM-VALUE>
                          </PARAMETER-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuSIRCClockConfig</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCDiv1</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCDiv1Frequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCDiv2</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCDiv2Frequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCFrequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCLowPowerEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCRangeSelect</DEFINITION-REF>
                          <VALUE>HIGH_RANGE_CLOCK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCStopEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSIRCClockConfig/McuSIRCUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuSystemOSCClockConfig</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCClockMonitorEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCClockMonitorResetEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCDiv1</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCDiv1Frequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCDiv2</DEFINITION-REF>
                          <VALUE>8</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCDiv2Frequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCExternalReferenceSelect</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCFrequency</DEFINITION-REF>
                          <VALUE>1.6E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCHighGainOscillatorSelect</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCRangeSelect</DEFINITION-REF>
                          <VALUE>HIGH_FREQ_RANGE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemOSCClockConfig/McuSOSCUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuSystemPll</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLClockMonitorEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLClockMonitorResetEnable</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLDiv1</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLDiv1Frequency</DEFINITION-REF>
                          <VALUE>9.6E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLDiv2</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLDiv2Frequency</DEFINITION-REF>
                          <VALUE>4.8E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLEnable</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLFrequency</DEFINITION-REF>
                          <VALUE>9.6E7</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLInputClkPreDivider</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLInputFrequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLMultiplier</DEFINITION-REF>
                          <VALUE>24</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSPLLSelectSourceClock</DEFINITION-REF>
                          <VALUE>SOSC_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuSystemPll/McuSystemPllUnderMcuControl</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuVlprClockConfig</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuBusClockDivider</DEFINITION-REF>
                          <VALUE>2</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuBusClockFrequency</DEFINITION-REF>
                          <VALUE>1000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuCoreClockDivider</DEFINITION-REF>
                          <VALUE>4</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuCoreClockFrequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuFlashClockFrequency</DEFINITION-REF>
                          <VALUE>500000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuPreDivSystemClockFrequency</DEFINITION-REF>
                          <VALUE>8000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuScgClkOutFrequency</DEFINITION-REF>
                          <VALUE>0.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuSlowClockDivider</DEFINITION-REF>
                          <VALUE>4</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuSystemClockFrequency</DEFINITION-REF>
                          <VALUE>2000000.0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuVlprClockConfig/McuSystemClockSwitch</DEFINITION-REF>
                          <VALUE>SIRC_CLK</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>McuInterruptEvents</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuInterruptEvents</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuInterruptEvents/McuAlternateResetEvent</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuInterruptEvents/McuVoltageErrorEvent</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>McuModeSettingConf_Run</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuModeSettingConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuModeSettingConf/McuEnableSleepOnExit</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuModeSettingConf/McuMode</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuModeSettingConf/McuPowerMode</DEFINITION-REF>
                      <VALUE>RUN</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>McuPowerControl</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuPowerControl</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuPowerControl/McuClockBiasDisable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuPowerControl/McuLPODisable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuPowerControl/McuLowPowerBiasEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuPowerControl/McuLowVoltageDetectInterruptEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuPowerControl/McuLowVoltageDetectResetEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuPowerControl/McuLowVoltageWarningInterruptEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>McuResetConfig</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuResetPinFilterBusClockSelect</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuResetPinFilterInRunAndWait</DEFINITION-REF>
                      <VALUE>ALL_FILTERING_DISABLE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuResetPinFilterInStopMode</DEFINITION-REF>
                      <VALUE>ALL_FILTERING_DISABLE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>McuSystemInterruptEnable</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuCMULossOfClockResetInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuCoreLockupInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuExternalResetPinInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuGlobalInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuJTAGResetInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuLossOfClockInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuLossOfLockInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuMDMAPSystemResetInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuResetDelayTime</DEFINITION-REF>
                          <VALUE>DELAY_10_LPO_CYCLES</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuSoftwareInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuStopAcknowledgeErrorInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuModuleConfiguration/McuResetConfig/McuSystemInterruptEnable/McuWatchdogInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>McuPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_CMU_LOSS_OF_CLOCK_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>8</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_CORE_LOCKUP_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>3</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_EXTERNAL_PIN_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>6</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_JTAG_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>4</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_LOSS_OF_CLOCK_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>10</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_LOSS_OF_LOCK_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>9</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_LOW_OR_HIGH_VOLTAGE_DETECT_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>11</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_MDM_AP_SYSTEM_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_MULTIPLE_RESET_REASON</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>13</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_NO_RESET_REASON</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>12</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_POWER_ON_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_RESET_UNDEFINED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>14</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_STOP_ACKNOWLEDGE_ERROR_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_SW_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>2</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_WATCHDOG_RESET</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/Mcu/McuPublishedInformation/McuResetReasonConf/McuResetReason</DEFINITION-REF>
                      <VALUE>7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
