<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00046.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>EcuM</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>EcuM</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T40D2M10I0R0/EcuM</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-POST-BUILD</IMPLEMENTATION-CONFIG-VARIANT>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>10</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>EcuMConfiguration</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>EcuMCommonConfiguration</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMConfigConsistencyHash</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMDefaultAppMode</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMOSResource</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>EcuMDefaultShutdownTarget</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMDefaultShutdownTarget</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMDefaultShutdownTarget/EcuMDefaultState</DEFINITION-REF>
                          <VALUE>EcuMStateSleep</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>EcuMSleepMode_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMSleepMode</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMSleepMode/EcuMSleepModeId</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMSleepMode/EcuMSleepModeSuspend</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-SYMBOLIC-NAME-REFERENCE-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMSleepMode/EcuMSleepModeMcuModeRef</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuModeSettingConf_Run</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-SYMBOLIC-NAME-REFERENCE-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMSleepMode/EcuMWakeupSourceMask</DEFINITION-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>EcuMWakeupSource_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource/EcuMWakeupSourceId</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource/EcuMWakeupSourcePolling</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>EcuMWakeupSource_1</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource/EcuMWakeupSourceId</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource/EcuMWakeupSourcePolling</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>EcuMGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D2M10I0R0/EcuM/EcuMGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMGeneral/EcuMDevErrorDetect</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMGeneral/EcuMIncludeDet</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMGeneral/EcuMMainFunctionPeriod</DEFINITION-REF>
                  <VALUE>1.0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D2M10I0R0/EcuM/EcuMGeneral/EcuMVersionInfoApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
