{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["表单","故障信息解析"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"表单","index":0,"n_rows":9,"n_cols":6,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["序号","名称","数据类型","精度","单位","备注"]
[1,"time_st","timestamps","s","%Y-%m-%d %H:%M:%S","故障开始时间"]
[2,"time_sp","timestamps","s","%Y-%m-%d %H:%M:%S","故障结束时间"]
[3,"sn","str","NA",null,"电池包编号"]
[4,"faultcode","int",1,null,"故障码"]
[5," faultlv","int",1,null,"故障等级"]
[6,"faultinfo","str","NA",null,"故障码对应的具体故障信息"]
[7,"faultadvice","str","NA",null,"故障处理建议"]
[8,"faultstate","int","NA",null,"故障处理状态"]

{"sheet":"故障信息解析","index":1,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[[4,7,6,7]]}
["故障码","故障码含义","故障等级","运维建议"]
[1,"数据通讯故障",2,"丢失电池信息，无法监控电池安全状态，请立刻检修电池采样系统及数据传输系统"]
[2,"温度无效",2,"丢失温度信息，无法全面监控电池安全；请停止充放电，并检修电池采样系统及数据传输系统"]
[4,"电芯高温",3,"高温下充放电，会导致容量衰减过快，存在热失控风险；请停止充放电，开启电池冷却功能，并通知电池技术人员介入分析",null,"故障等级","说明","建议"]
[6,"电芯低温",3,"低温下充电，会导致析锂，存在电池安全与寿命衰减过快风险；请停止充放电，并开启电池加热功能",null,1,"电池状态估计故障，对健康度有影响，可能产生安全风险","提示并作出相应动作"]
[8,"温差过大",3,"存在电芯的老化速率不一致的风险；请检查电池温度采样系统",null,2,"电池通讯或采样故障，失去对电池的安全监控"]
[9,"温升过快",3,"温升速率过快，存在热失控风险；禁止充放电，并通知电池技术人员介入分析",null,3,"电池存在影响安全的动作"]
[10,"电压断线",2,"丢失部分电压信息，无法全面监控电池安全；禁止充放电，请检查电池电压采样系统",null,4,"电池存在安全隐患"]
[12,"单体过压",3,"过压可能导致电池析锂，存在电池安全与寿命衰减过快风险；禁止充电，若持续>10min，请通知电池技术人员介入分析",null,5,"电池发生安全事故"]
[14,"单体欠压",3,"欠压可能导致电池过放；禁止放电，请充电，若欠压持续>10min，通知电池技术人员介入分析"]
[16,"压差过大",3,"电量/内阻不一致；请均衡电池，若均衡无法解决问题，请通知电池技术人员介入分析"]
[18,"总压过压",3,"过压会导致电池析锂，存在电池安全与寿命衰减过快风险；请停止充电，若过压持续>10min，通知电池技术人员介入分析"]
[20,"总压欠压",3,"欠压可能导致电池过放；请停止放电，并充电，若欠压持续>10min，请通知电池技术人员介入分析"]
[21,"充电过流",3,"过流会导致电池析锂，存在电池安全与寿命衰减过快风险；请停止充电，若持续>5min，断开继电器，并通知电池技术人员介入分析"]
[22,"放电过流",3,"长时间过流会导致电池欠压及温升过快；请停止放电，若持续>5min，断开继电器，并通知电池技术人员介入分析"]
[23,"容量过低",1,"电池容量过低，会导致电池放电电量不足；建议更换容量过低的电芯或模组"]
[24,"容量一致性差",1,"电池容量不一致性差，会导致电池放电电量不足；建议更换容量过低的电芯或模组"]
[25,"SOC一致性差",1,"请均衡电池，若无法解决，请通知电池技术人员介入分析"]
[26,"低电量报警",1,"电量过低会引起电池过放；请停止放电，并充电"]
[27,"SOC卡滞",1,"请通知电池供应商检查电池BMS软件是否正常"]
[28,"SOC跳变",1,"请通知电池供应商检查电池BMS软件是否正常"]
[29,"SOC误差过大",1,"请通知电池供应商检查电池BMS软件是否正常"]
[100,"长时间未标定",1,"电池长时间未标定，存在电池状态估算不准确风险，请对电池进行：放电至SOC<10%-静置1.5h-充满，操作"]
[110,"热失控预警",4,"断开继电器，远离电池，并通知电池技术人员介入分析"]
[119,"热失控报警",5,"断开继电器，远离电池，立刻消防处理，并通知技术人员介入"]