-std=c99
-DCPU_S32K144HFT0VLLT
-DI_CACHE_ENABLE
-DENABLE_FPU
-DGCC
-DS32K1XX
-DS32K144
-I../RTD/include
-I../FreeRTOS/Source/include
-I"D:/1_WorkFiles/2_Software/11.Communicator/workspace/S32K144_BLE/FreeRTOS/Source/include"
-I"D:/1_WorkFiles/2_Software/11.Communicator/workspace/S32K144_BLE/FreeRTOS/Source/portable/GCC/ARM_CM4F"
-ID:/1_WorkFiles/2_Software/11.Communicator/workspace/S32K144_BLE/generate/include
-ID:/1_WorkFiles/2_Software/11.Communicator/workspace/S32K144_BLE/RTD/include
-I"D:/1_WorkFiles/2_Software/11.Communicator/workspace/S32K144_BLE/board"
-I"C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/header"
-I"C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Base_TS_T40D2M10I0R0/include"
-I"C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Platform_TS_T40D2M10I0R0/include"
-I"C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K1_2021_08/SW32K1_RTD_4_4_1_0_0_D2108/Platform_TS_T40D2M10I0R0/startup/include"
-O0
-funsigned-char
-fstack-usage
-fdump-ipa-all
-fomit-frame-pointer
-ggdb3
-pedantic
-Wall
-Wextra
-c
-fno-short-enums
-funsigned-bitfields
-fno-common
-Wunused
-Wstrict-prototypes
-Wsign-compare
-Werror=implicit-function-declaration
-Wundef
-Wdouble-promotion
-mcpu=cortex-m4
-mthumb
-mlittle-endian
-mfloat-abi=hard
-mfpu=fpv4-sp-d16
-specs=nano.specs
-specs=nosys.specs
--sysroot="C:/NXP/S32DS.3.4/S32DS/build_tools/gcc_v9.2/gcc-9.2-arm32-eabi/arm-none-eabi/newlib"