
Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Symbol table:

Can_ProcessBusOffInterrupt/3 (Can_ProcessBusOffInterrupt) @070237e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Can_ErrorIrqCallback/1 
  Calls: 
Can_ProcessPNInterrupt/2 (Can_ProcessPNInterrupt) @07023620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags:
  Called by: Can_CommonIrqCallback/0 
  Calls: 
Can_ErrorIrqCallback/1 (Can_ErrorIrqCallback) @070231c0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Can_ProcessBusOffInterrupt/3 
Can_CommonIrqCallback/0 (Can_CommonIrqCallback) @0701bee0
  Type: function definition analyzed
  Visibility: force_output externally_visible no_reorder public
  References: 
  Referring: 
  Availability: available
  Function flags: body
  Called by: 
  Calls: Can_ProcessPNInterrupt/2 
Can_ErrorIrqCallback (uint8 u8Instance, Flexcan_Ip_EventType event, uint32 u32ErrStatus, const struct Flexcan_Ip_StateType * driverState)
{
  <bb 2> :
  if (event_2(D) == 9)
    goto <bb 3>; [INV]
  else
    goto <bb 4>; [INV]

  <bb 3> :
<L0>:
  Can_ProcessBusOffInterrupt (u8Instance_4(D));
  goto <bb 5>; [INV]

  <bb 4> :
<L1>:

  <bb 5> :
  return;

}


Can_CommonIrqCallback (uint8 u8Instance, Flexcan_Ip_EventType event, uint32 u32buffIdx, const struct Flexcan_Ip_StateType * driverState)
{
  <bb 2> :
  if (event_2(D) == 6)
    goto <bb 3>; [INV]
  else
    goto <bb 4>; [INV]

  <bb 3> :
  Can_ProcessPNInterrupt (u8Instance_4(D));

  <bb 4> :
  return;

}


