{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":8,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["product_id","start_time","end_time","code","level","info","advice","Batpos"]
["PK504B10100004429","2021-11-08T19:44:00","0000-00-00 00:00:00",50,3,"单体电压大于4.00V,采样无效","建议返厂维修",0]
["PK504B10100004429","2021-11-08T19:22:00","2021-11-09T19:32:00",50,3,"单体电压大于4.00V,采样无效","建议返厂维修",1]
[{"$nulls":7},"0代表车辆需要处理\n1代表车辆已处理"]