{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[3.4336000000000002,100,3.4336000000000002,100]
["3.335.3",95,"3.335.3",95]
[3.3330000000000002,90,3.3330000000000002,90]
[3.3313999999999999,85,3.3313999999999999,85]
[3.3302,80,3.3302,80]
[3.32945,75,3.32945,75]
[3.3285999999999998,70,3.3285999999999998,70]
[3.3281499999999999,65,3.3281499999999999,65]
[3.3224,60,3.3224,60]
[3.2976000000000001,55,3.2976000000000001,55]
[3.2922500000000001,50,3.2922500000000001,50]
[3.2905000000000002,45,3.2905000000000002,45]
[3.2892999999999999,40,3.2892999999999999,40]
[3.2883,35,3.2883,35]
[3.28505,30,3.28505,30]
[3.2695500000000002,25,3.2695500000000002,25]
[3.2531500000000002,20,3.2531500000000002,20]
[3.2275499999999999,15,3.2275499999999999,15]
[3.20505,10,3.20505,10]
[3.1815000000000002,5,3.1815000000000002,5]
[2.78315,0,2.78315,0]