{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[3.4461500000000003,100,3.4461500000000003,100]
[3.3347499999999997,95,3.3347499999999997,95]
[3.3324499999999997,90,3.3324499999999997,90]
[3.3307000000000002,85,3.3307000000000002,85]
[3.3295500000000002,80,3.3295500000000002,80]
[3.3288500000000001,75,3.3288500000000001,75]
[3.3285499999999999,70,3.3285499999999999,70]
[3.3282499999999997,65,3.3282499999999997,65]
[3.32565,60,3.32565,60]
[3.2966499999999996,55,3.2966499999999996,55]
[3.29135,50,3.29135,50]
[3.2897499999999997,45,3.2897499999999997,45]
[3.28905,40,3.28905,40]
[3.2882499999999997,35,3.2882499999999997,35]
[3.2862,30,3.2862,30]
[3.2697500000000002,25,3.2697500000000002,25]
[3.2530999999999999,20,3.2530999999999999,20]
[3.2295499999999997,15,3.2295499999999997,15]
[3.2049500000000002,10,3.2049500000000002,10]
[3.1812499999999999,5,3.1812499999999999,5]
[2.8327999999999998,0,2.8327999999999998,0]