{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[3.4264749999999999,100,3.4893049999999999,100]
[3.3319799999999997,95,3.3381850000000002,95]
[3.3301600000000002,90,3.3367800000000001,90]
[3.3281749999999999,80,3.3363199999999997,80]
[3.32674,70,3.3357049999999999,70]
[3.3026299999999997,60,3.312195,60]
[3.2874499999999998,50,3.3065249999999997,50]
[3.2868550000000001,40,3.3026999999999997,40]
[3.2819349999999998,30,3.2996150000000002,30]
[3.2467899999999998,20,3.2717200000000002,20]
[3.2051949999999998,10,3.219735,10]
[3.1481050000000002,5,3.1795849999999999,5]
[2.7375949999999998,0,2.7890299999999999,0]