{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[3.4359500000000001,100,3.4359500000000001,100]
[3.3348,95,3.3348,95]
[3.33325,90,3.33325,90]
[3.3316499999999998,85,3.3316499999999998,85]
[3.3302499999999999,80,3.3302499999999999,80]
[3.3294000000000001,75,3.3294000000000001,75]
[3.3288500000000001,70,3.3288500000000001,70]
[3.3285,65,3.3285,65]
[3.3173499999999998,60,3.3173499999999998,60]
[3.2944499999999999,55,3.2944499999999999,55]
[3.2913000000000001,50,3.2913000000000001,50]
[3.2902499999999999,45,3.2902499999999999,45]
[3.28945,40,3.28945,40]
[3.2888999999999999,35,3.2888999999999999,35]
[3.2854000000000001,30,3.2854000000000001,30]
[3.2675000000000001,25,3.2675000000000001,25]
[3.2517499999999999,20,3.2517499999999999,20]
[3.2281,15,3.2281,15]
[3.2052499999999999,10,3.2052499999999999,10]
[3.1812499999999999,5,3.1812499999999999,5]
[2.8328000000000002,0,2.8328000000000002,0]