{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.3170000000000002,100,4.3170000000000002,100]
[4.2359999999999998,95,4.2359999999999998,95]
[4.1790000000000003,90,4.1790000000000003,90]
[4.1219999999999999,85,4.1219999999999999,85]
[4.0629999999999997,80,4.0629999999999997,80]
[4.0039999999999996,75,4.0039999999999996,75]
[3.9470000000000001,70,3.9470000000000001,70]
[3.8919999999999999,65,3.8919999999999999,65]
[3.839,60,3.839,60]
[3.79,55,3.79,55]
[3.7309999999999999,50,3.7309999999999999,50]
[3.6949999999999998,45,3.6949999999999998,45]
[3.6720000000000002,40,3.6720000000000002,40]
[3.653,35,3.653,35]
[3.637,30,3.637,30]
[3.6219999999999999,25,3.6219999999999999,25]
[3.6,20,3.6,20]
[3.5670000000000002,15,3.5670000000000002,15]
[3.5339999999999998,10,3.5339999999999998,10]
[3.4910000000000001,5,3.4910000000000001,5]
[3.42,0,3.42,0]