{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.3247,100,4.3247,100]
[4.2258000000000004,95,4.2258000000000004,95]
[4.1811999999999996,90,4.1811999999999996,90]
[4.1378000000000004,85,4.1378000000000004,85]
[4.0838000000000001,80,4.0838000000000001,80]
[4.0255999999999998,75,4.0255999999999998,75]
[3.9681999999999999,70,3.9681999999999999,70]
[3.9136000000000002,65,3.9136000000000002,65]
[3.8591000000000002,60,3.8591000000000002,60]
[3.8035999999999999,55,3.8035999999999999,55]
[3.7347999999999999,50,3.7347999999999999,50]
[3.6928999999999998,45,3.6928999999999998,45]
[3.6680999999999999,40,3.6680999999999999,40]
[3.6488999999999998,35,3.6488999999999998,35]
[3.6318000000000001,30,3.6318000000000001,30]
[3.6139000000000001,25,3.6139000000000001,25]
[3.5834999999999999,20,3.5834999999999999,20]
[3.5463,15,3.5463,15]
[3.4982000000000002,10,3.4982000000000002,10]
[3.4550999999999998,5,3.4550999999999998,5]
[3.4011999999999998,0,3.4011999999999998,0]