{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.3294350000000001,100,4.3202480000000003,100]
[4.2310290000000004,95,4.2291460000000001,95]
[4.17943,90,4.176126,90]
[4.1270069999999999,85,4.1226859999999999,85]
[4.0698730000000003,80,4.0647919999999997,80]
[4.0111350000000003,75,4.0056070000000004,75]
[3.9540609999999998,70,3.9485389999999998,70]
[3.899632,65,3.8931290000000001,65]
[3.8458399999999999,60,3.8372419999999998,60]
[3.7891349999999999,55,3.7810540000000001,55]
[3.7281840000000002,50,3.722283,50]
[3.695084,45,3.6868430000000001,45]
[3.6721720000000002,40,3.6638890000000002,40]
[3.6544859999999999,35,3.6463589999999999,35]
[3.6392859999999998,30,3.6306029999999998,30]
[3.6241979999999998,25,3.6129660000000001,25]
[3.6042510000000001,20,3.5829879999999998,20]
[3.5687129999999998,15,3.5496560000000001,15]
[3.5213429999999999,10,3.5079090000000002,10]
[3.4751430000000001,5,3.4669660000000002,5]
[3.395,0,3.4089999999999998,0]