{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":4,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.1660000000000004,100,4.1660000000000004,100]
[4.1059999999999999,95,4.1059999999999999,95]
[4.0810000000000004,90,4.0810000000000004,90]
[4.0430000000000001,85,4.0430000000000001,85]
[3.9889999999999999,80,3.9889999999999999,80]
[3.9889999999999999,75,3.9889999999999999,75]
[3.899,70,3.899,70]
[3.859,65,3.859,65]
[3.8109999999999999,60,3.8109999999999999,60]
[3.7450000000000001,55,3.7450000000000001,55]
[3.69,50,3.69,50]
[3.6539999999999999,45,3.6539999999999999,45]
[3.6269999999999998,40,3.6269999999999998,40]
[3.6030000000000002,35,3.6030000000000002,35]
[3.5779999999999998,30,3.5779999999999998,30]
[3.5470000000000002,25,3.5470000000000002,25]
[3.5019999999999998,20,3.5019999999999998,20]
[3.452,15,3.452,15]
[3.3940000000000001,10,3.3940000000000001,10]
[3.35,5,3.35,5]
[3.3330000000000002,3,3.3330000000000002,3]
[3.2,0,3.2,0]