{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.2722499999999997,100,4.2722499999999997,100]
[4.1886500000000009,95,4.1886500000000009,95]
[4.1235499999999998,90,4.1235499999999998,90]
[4.0600000000000005,85,4.0600000000000005,85]
[3.9988000000000001,80,3.9988000000000001,80]
[3.9413,75,3.9413,75]
[3.8865500000000002,70,3.8865500000000002,70]
[3.8327999999999998,65,3.8327999999999998,65]
[3.7783499999999997,60,3.7783499999999997,60]
[3.7112499999999997,55,3.7112499999999997,55]
[3.6704499999999998,50,3.6704499999999998,50]
[3.6453499999999996,45,3.6453499999999996,45]
[3.6263000000000001,40,3.6263000000000001,40]
[3.6093999999999999,35,3.6093999999999999,35]
[3.5909499999999999,30,3.5909499999999999,30]
[3.5593000000000004,25,3.5593000000000004,25]
[3.5217999999999998,20,3.5217999999999998,20]
[3.4752999999999998,15,3.4752999999999998,15]
[3.4313000000000002,10,3.4313000000000002,10]
[3.3840500000000002,5,3.3840500000000002,5]
[3.1597499999999998,0,3.1597499999999998,0]