{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.2317999999999998,100,4.2317999999999998,100]
[4.1684000000000001,95,4.1684000000000001,95]
[4.1234000000000002,90,4.1234000000000002,90]
[4.0709,85,4.0709,85]
[4.0151000000000003,80,4.0151000000000003,80]
[3.9609999999999999,75,3.9609999999999999,75]
[3.9098000000000002,70,3.9098000000000002,70]
[3.8586999999999998,65,3.8586999999999998,65]
[3.8060999999999998,60,3.8060999999999998,60]
[3.7425000000000002,55,3.7425000000000002,55]
[3.6884000000000001,50,3.6884000000000001,50]
[3.6593,45,3.6593,45]
[3.6387999999999998,40,3.6387999999999998,40]
[3.6217000000000001,35,3.6217000000000001,35]
[3.6048,30,3.6048,30]
[3.5794000000000001,25,3.5794000000000001,25]
[3.5413000000000001,20,3.5413000000000001,20]
[3.4983,15,3.4983,15]
[3.4472999999999998,10,3.4472999999999998,10]
[3.4134000000000002,5,3.4134000000000002,5]
[3.2719,0,3.2719,0]