{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[3379,100,3379,100]
[3331.333333333333,95,3331.333333333333,95]
[3329.42,90,3329.42,90]
[3328.9466666666667,85,3328.9466666666667,85]
[3328.5466666666666,80,3328.5466666666666,80]
[3328.186666666666,75,3328.186666666666,75]
[3327.4533333333334,70,3327.4533333333334,70]
[3325.143333333333,65,3325.143333333333,65]
[3315.1733333333327,60,3315.1733333333327,60]
[3299.7166666666662,55,3299.7166666666662,55]
[3292.29,50,3292.29,50]
[3289.9066666666668,45,3289.9066666666668,45]
[3288.8233333333333,40,3288.8233333333333,40]
[3287.96,35,3287.96,35]
[3285.48,30,3285.48,30]
[3274.3533333333335,25,3274.3533333333335,25]
[3258.0533333333333,20,3258.0533333333333,20]
[3237.353333333333,15,3237.353333333333,15]
[3211.3466666666668,10,3211.3466666666668,10]
[3182.2733333333331,5,3182.2733333333331,5]
[2995.3666666666668,0,2995.3666666666668,0]