{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.1379999999999999,100,4.1319999999999997,100]
[4.0919999999999996,94.107227144146407,4.0860000000000003,94.107227144146407]
[4.05,89.168154849392096,4.0430000000000001,89.168154849392096]
[3.95,79.290732355878305,3.9409999999999998,79.290732355878305]
[3.8639999999999999,69.413538571699704,3.855,69.413538571699704]
[3.7770000000000001,59.536426272695401,3.7679999999999998,59.536426272695401]
[3.6850000000000001,49.659312505979997,3.6720000000000002,49.659312505979997]
[3.6440000000000001,39.7822390922734,3.63,39.7822390922734]
[3.6110000000000002,29.9053673711329,3.5960000000000001,29.9053673711329]
[3.5569999999999999,20.028514766482498,3.536,20.028514766482498]
[3.4569999999999999,10.1515649123484,3.4369999999999998,10.1515649123484]
[3.4209999999999998,5.2128308979418696,3.399,5.2128308979418696]
[3.173,0,3.1539999999999999,0]