{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.2890220000000001,100,4.2808679999999999,100]
[4.2130219999999996,95,4.2150220000000003,95]
[4.1630070000000003,90,4.1670220000000002,90]
[4.1090070000000001,85,4.114134,85]
[4.0518910000000004,80,4.0580220000000002,80]
[3.9940069999999999,75,4.0010219999999999,75]
[3.940007,70,3.947022,70]
[3.8870070000000001,65,3.895022,65]
[3.8360069999999999,60,3.8440219999999998,60]
[3.787007,55.000000000000007,3.7950050000000002,55.000000000000007]
[3.723007,50,3.7300219999999999,50]
[3.6880069999999998,45,3.6980219999999999,45]
[3.666007,40,3.6760220000000001,40]
[3.6490070000000001,35,3.6585960000000002,35]
[3.634007,30,3.6430280000000002,30]
[3.6180129999999999,25,3.628746,25]
[3.5910069999999998,20,3.6100219999999998,20]
[3.557007,15,3.576022,15]
[3.5150070000000002,10,3.5320070000000001,10]
[3.4710070000000002,5,3.4816704999999999,5,null,"`"]
[3.436007,0,3.436007,0]