{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.2628462314605713,100,4.2628462314605713,100]
[4.170265483856201,95,4.170265483856201,95]
[4.1059548854827881,90,4.1059548854827881,90]
[4.0448836326599125,85,4.0448836326599125,85]
[3.9876305580139162,80,3.9876305580139162,80]
[3.9346242427825926,75,3.9346242427825926,75]
[3.8839908599853517,70,3.8839908599853517,70]
[3.8340200185775757,65,3.8340200185775757,65]
[3.7828853607177733,60,3.7828853607177733,60]
[3.7256537437438966,55,3.7256537437438966,55]
[3.6813785552978517,50,3.6813785552978517,50]
[3.6547574996948242,45,3.6547574996948242,45]
[3.635063648223877,40,3.635063648223877,40]
[3.6182509660720825,35,3.6182509660720825,35]
[3.6024014472961428,30,3.6024014472961428,30]
[3.584269142150879,25,3.584269142150879,25]
[3.5507390975952147,20,3.5507390975952147,20]
[3.512633204460144,15,3.512633204460144,15]
[3.4626659393310546,10,3.4626659393310546,10]
[3.4333167672157288,5,3.4333167672157288,5]
[3.3858912467956541,0,3.3858912467956541,0]