{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":25,"n_cols":4,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["充电OCV","充电SOC","放电OCV","放电SOC"]
[4.2729999999999997,100,4.2729999999999997,100]
[4.2229999999999999,97,4.2229999999999999,97]
[4.1900000000000004,95,4.1900000000000004,95]
[4.1289999999999996,90,4.1289999999999996,90]
[4.07,85,4.07,85]
[4.0119999999999996,80,4.0119999999999996,80]
[3.9569999999999999,75,3.9569999999999999,75]
[3.9049999999999998,70,3.9049999999999998,70]
[3.8540000000000001,65,3.8540000000000001,65]
[3.8069999999999999,60,3.8069999999999999,60]
[3.7589999999999999,55,3.7589999999999999,55]
[3.71,50,3.71,50]
[3.681,45,3.681,45]
[3.661,40,3.661,40]
[3.645,35,3.645,35]
[3.63,30,3.63,30]
[3.6150000000000002,25,3.6150000000000002,25]
[3.5840000000000001,20,3.5840000000000001,20]
[3.5539999999999998,15,3.5539999999999998,15]
[3.5179999999999998,10,3.5179999999999998,10]
[3.4750000000000001,5,3.4750000000000001,5]
[3.4580000000000002,3,3.4580000000000002,3]
[3.4409999999999998,1,3.4409999999999998,1]
[3.4329999999999998,0,3.4329999999999998,0]